| Home > Technical Specifications # Scanner Specifications General Mechanical Electrical Environmental Interfaces Standards and Approvals Note:
Specifications are subject to change without notice.
## General
Scanner type | Flatbed color
Photoelectric device | Color CCD line sensor
Effective pixels | 54400 × 74880 pixels at 6400 dpi Scanning area may be restricted if resolution setting is large.
Document size | Reflective: 216 × 297 mm (8.5 × 11.7 inches) A4 or US letter size Transparent: 35 mm film strip: 12 frames at a time 35 mm slides: up to 4 slides at a time 6 cm medium format: up to 22 cm
Scanning resolution | 6400 dpi (main scan) 9600 dpi with Micro Step (sub scan)
Output resolution | 50 to 6400, 9600, and 12800 dpi (50 to 6400 dpi in 1 dpi increments)
Image data | 16 bits per pixel per color internal 16 bits per pixel per color external (maximum)
Interface | One USB 2.0 Hi-speed/USB 1.1 port
Light source | White LED, IR LED
Note:
Optional optical resolution is the maximum scan resolution of the CCD elements, using the definition of ISO 14473. ISO 14473 defines optical resolution as the fundamental sampling rate of the scan sensor.
Top ## Mechanical
Dimensions | Width: 280 mm (11.0 inches) Depth: 485 mm (19.1 inches) Height: 118 mm (4.6 inches)
Weight | Approx. 4.1 kg (9.0 lb) without AC adaptor
Top ## Electrical Note:
Check the label on the AC adapter or on the back of the scanner for voltage information.
### Scanner
Rated voltage | DC 24 V
Rated input current | 1.3 A
Power consumption | 16.5 W Operating 5.5 W Ready Mode 1.6 W Sleep Mode 0.4 W Power off
### AC Adapter
| 100-120 V model | 220-240 V model
AC adapter model | A411B | A411E
Rated input voltage | AC 100 to 120 V | AC 220 to 240 V
Rated input current | 1.0 A | 0.5 A
Rated input frequency | 50 to 60 Hz
Rated output voltage | DC 24 V
Rated output current | 1.3 A
Note:
The AC adapter model varies in certain locations.
Top ## Environmental
Temperature | Operating | 10 to 35 ˚C (50 to 95 ˚F)
Storage | –25 to 60 ˚C (–13 to 140 ˚F)
Humidity | Operating | 10 to 80%, without condensation
Storage | 10 to 85%, without condensation
Operating conditions | Ordinary office or home conditions. Avoid operating the scanner in direct sunlight, near a strong light source, or in extremely dusty conditions.
Top ## Interfaces ### USB Interface
Interface type | Universal Serial Bus Specification Revision 2.0
Electrical standard | Full Speed mode (12 Mbits per second) and Hi-Speed mode (480 Mbits per second) of Universal Serial Bus Specification Revision 2.0.
Connector type | One Type B port
Top ## Standards and Approvals ### Scanner U.S. model:
EMC | FCC Part 15 Subpart B Class B CAN/CSA-CEI/IEC CISPR22 Class B
European model:
EMC Directive 2004/108/EC | EN 55022 Class B EN 55024
Australian model:
EMC | AS/NZS CISPR22 Class B
### AC Adapter U.S. model:
Safety | UL60950-1 CAN/CSA-C22.2 No. 60950-1
EMC | FCC Part 15 Subpart B Class B CAN/CSA-CEI/IEC CISPR22 Class B
European model:
Low Voltage Directive 2006/95/EC EMC Directive 2004/108/EC | EN 60950-1 EN 55022 Class B EN 55024 EN 61000-3-2 EN 61000-3-3
Australian model:
Safety | AS/NZS 60950.1
EMC | AS/NZS CISPR22 Class B
Top |