
			Generic serial MIDI driver
			==========================

The snd_adaptor module parameter allows you to select either:

  0 - Roland Soundcanvas support (default)
  1 - Midiator MS-124T support (1)
  2 - Midiator MS-124W S/A mode (2)
  3 - MS-124W M/B mode support (3)

For the Midiator MS-124W, you must set the physical M-S and A-B
switches on the Midiator to match the driver mode you select.

In Roland Soundcanvas mode, multiple ALSA raw MIDI substreams are supported
(midiCnD0-midiCnD15).  Whenever you write to a different substream, the driver
sends the nonstandard MIDI command sequence F5 NN, where NN is the substream
number plus 1.  Roland modules use this command to switch between different
"parts", so this feature lets you treat each part as a distinct raw MIDI
substream. The driver provides no way to send F5 00 (no selection) or to not
send the F5 NN command sequence at all; perhaps it ought to.

Usage example for simple serial converter:

	/sbin/modprobe snd-serialmidi snd_sdev="/dev/ttyS0"

Usage example for Roland SoundCanvas with 4 MIDI ports:

	/sbin/modprobe snd-serialmidi snd_sdev="/dev/ttyS0" snd_outs=4

In MS-124T mode, one raw MIDI substream is supported (midiCnD0); the snd_outs
module parameter is automatically set to 1. The driver sends the same data to
all four MIDI Out connectors.  Set the A-B switch and the snd_speed module
parameter to match (A=19200, B=9600).

Usage example for MS-124T, with A-B switch in A position:

	/sbin/modprobe snd-serialmidi snd_sdev="/dev/ttyS0" \
			snd_adaptor=1 snd_speed=19200

In MS-124W S/A mode, one raw MIDI substream is supported (midiCnD0);
the snd_outs module parameter is automatically set to 1. The driver sends
the same data to all four MIDI Out connectors at full MIDI speed.

Usage example for S/A mode:

	/sbin/modprobe snd-serialmidi snd_sdev="/dev/ttyS0" \
			snd_adaptor=2

In MS-124W M/B mode, the driver supports 16 ALSA raw MIDI substreams;
the snd_outs module parameter is automatically set to 16.  The substream
number gives a bitmask of which MIDI Out connectors the data should be
sent to, with midiCnD1 sending to Out 1, midiCnD2 to Out 2, midiCnD4 to
Out 3, and midiCnD8 to Out 4.  Thus midiCnD15 sends the data to all 4 ports.
As a special case, midiCnD0 also sends to all ports, since it is not useful
to send the data to no ports.  M/B mode has extra overhead to select the MIDI
Out for each byte, so the aggregate data rate across all four MIDI Outs is
at most one byte every 520 us, as compared with the full MIDI data rate of
one byte every 320 us per port.

Usage example for M/B mode:

	/sbin/modprobe snd-serialmidi snd_sdev="/dev/ttyS0" \
			snd_adaptor=3

The MS-124W hardware's M/A mode is currently not supported. This mode allows
the MIDI Outs to act independently at double the aggregate throughput of M/B,
but does not allow sending the same byte simultaneously to multiple MIDI Outs. 
The M/A protocol requires the driver to twiddle the modem control lines under
timing constraints, so it would be a bit more complicated to implement than
the other modes.

Midiator models other than MS-124W and MS-124T are currently not supported. 
Note that the suffix letter is significant; the MS-124 and MS-124B are not
compatible, nor are the other known models MS-101, MS-101B, MS-103, and MS-114.
I do have documentation (tim.mann@compaq.com) that partially covers these models,
but no units to experiment with.  The MS-124W support is tested with a real unit.
The MS-124T support is untested, but should work.
