#
# VICE definition file for HotKeys in Win32
#
# This version is for x64.
#
# Syntax:
# First column: string identifier
# Second column: iso language identifier
# Third column: hotkey character
# Fourth column: which occurence of the hotkey character to use
#                if no occurence is given the first occurence
#                is assumed

# res.rc

IDS_ATTACH					en	A	1
IDS_ATTACH					da	T	1
IDS_ATTACH					de	E	1
IDS_ATTACH					fr	I	1
IDS_ATTACH					hu	C	1
IDS_ATTACH					it	S	1
IDS_ATTACH					nl	K	1
IDS_ATTACH					sv	A	1
IDS_ATTACH					tr	Y	1

IDS_BROWSE					en	B	1
IDS_BROWSE					da	G	1
IDS_BROWSE					de	b	1
IDS_BROWSE					fr	P	1
IDS_BROWSE					hu	T	1
IDS_BROWSE					it	S	1
IDS_BROWSE					nl	B	1
IDS_BROWSE					sv	B	1
IDS_BROWSE					tr	G	1

IDS_DATASETTE_RESET_WITH_CPU	en	R	1
IDS_DATASETTE_RESET_WITH_CPU	da	R	1
IDS_DATASETTE_RESET_WITH_CPU	de	r	1
IDS_DATASETTE_RESET_WITH_CPU	fr	R	1
IDS_DATASETTE_RESET_WITH_CPU	hu	A	1
IDS_DATASETTE_RESET_WITH_CPU	it	R	1
IDS_DATASETTE_RESET_WITH_CPU	nl	R	1
IDS_DATASETTE_RESET_WITH_CPU	sv	N	1
IDS_DATASETTE_RESET_WITH_CPU	tr	r	2

IDS_DATASETTE_DELAY_TRIGGER	en	d	3
IDS_DATASETTE_DELAY_TRIGGER	da	f	1
IDS_DATASETTE_DELAY_TRIGGER	de	d	1
IDS_DATASETTE_DELAY_TRIGGER	fr	d	3
IDS_DATASETTE_DELAY_TRIGGER	sv	f	1

IDS_DATASETTE_DELAY_AT_ZERO	en	z	1
IDS_DATASETTE_DELAY_AT_ZERO	da	n	2
IDS_DATASETTE_DELAY_AT_ZERO	de	Z	2
IDS_DATASETTE_DELAY_AT_ZERO	fr	z	1
IDS_DATASETTE_DELAY_AT_ZERO	hu	n	2
IDS_DATASETTE_DELAY_AT_ZERO	it	z	1
IDS_DATASETTE_DELAY_AT_ZERO	nl	n	1
IDS_DATASETTE_DELAY_AT_ZERO	sv	n	3
IDS_DATASETTE_DELAY_AT_ZERO	tr	g	1

IDS_TOGGLE_USEIECDEVICE		en	U	1
IDS_TOGGLE_USEIECDEVICE		da	A	1
IDS_TOGGLE_USEIECDEVICE		de	a	1
IDS_TOGGLE_USEIECDEVICE		fr	U	1
IDS_TOGGLE_USEIECDEVICE		hu	I	1
IDS_TOGGLE_USEIECDEVICE		it	U	1
IDS_TOGGLE_USEIECDEVICE		nl	G	1
IDS_TOGGLE_USEIECDEVICE		sv	A	1
IDS_TOGGLE_USEIECDEVICE		tr	u	1

IDS_SELECTDISK				en	i	2
IDS_SELECTDISK				da	i	2
IDS_SELECTDISK				de	I	1
IDS_SELECTDISK				fr	I	1
IDS_SELECTDISK				hu	k	1
IDS_SELECTDISK				it	I	1
IDS_SELECTDISK				nl	b	1
IDS_SELECTDISK				sv	a	1
IDS_SELECTDISK				tr	i	2

IDS_SELECTDIR				en	D	1
IDS_SELECTDIR				da	K	1
IDS_SELECTDIR				de	D	1
IDS_SELECTDIR				fr	R	1
IDS_SELECTDIR				hu	n	1
IDS_SELECTDIR				it	D	1
IDS_SELECTDIR				nl	D	1
IDS_SELECTDIR				sv	K	1
IDS_SELECTDIR				tr	D	1

IDS_SELECTREAL				en	l	1
IDS_SELECTREAL				da	Æ	1
IDS_SELECTREAL				de	l	1
IDS_SELECTREAL				hu	V	1
IDS_SELECTREAL				it	l	1
IDS_SELECTREAL				nl	r	1
IDS_SELECTREAL				sv	Ä	1
IDS_SELECTREAL				tr	r	1

IDS_SELECTNONE				en	N	1
IDS_SELECTNONE				da	I	1
IDS_SELECTNONE				de	n	1
IDS_SELECTNONE				fr	A	1
IDS_SELECTNONE				hu	N	1
IDS_SELECTNONE				it	N	1
IDS_SELECTNONE				nl	e	1
IDS_SELECTNONE				sv	I	1
IDS_SELECTNONE				tr	Y	1

IDS_AUTOSTART				**	A	1
IDS_AUTOSTART				fr	D	1
IDS_AUTOSTART				sv	a	3
IDS_AUTOSTART				tr	a	1

IDS_BROWSEDIR				en	w	1
IDS_BROWSEDIR				da	G	1
IDS_BROWSEDIR				de	b	1
IDS_BROWSEDIR				fr	r	1
IDS_BROWSEDIR				hu	T	1
IDS_BROWSEDIR				it	S	1
IDS_BROWSEDIR				nl	d	1
IDS_BROWSEDIR				sv	B	1
IDS_BROWSEDIR				tr	G	1

IDS_TOGGLE_READP00			**	L	1
IDS_TOGGLE_READP00			en	R	1
IDS_TOGGLE_READP00			hu	b	1
IDS_TOGGLE_READP00			tr	r	1

IDS_TOGGLE_WRITEP00			en	W	1
IDS_TOGGLE_WRITEP00			da	S	1
IDS_TOGGLE_WRITEP00			de	S	1
IDS_TOGGLE_WRITEP00			fr	É	1
IDS_TOGGLE_WRITEP00			hu	m	1
IDS_TOGGLE_WRITEP00			it	S	1
IDS_TOGGLE_WRITEP00			nl	S	1
IDS_TOGGLE_WRITEP00			sv	S	1
IDS_TOGGLE_WRITEP00			tr	y	2

IDS_TOGGLE_HIDENONP00			en	H	1
IDS_TOGGLE_HIDENONP00			da	G	1
IDS_TOGGLE_HIDENONP00			de	a	2
IDS_TOGGLE_HIDENONP00			fr	C	1
IDS_TOGGLE_HIDENONP00			hu	e	2
IDS_TOGGLE_HIDENONP00			it	N	1
IDS_TOGGLE_HIDENONP00			nl	V	1
IDS_TOGGLE_HIDENONP00			sv	G	1
IDS_TOGGLE_HIDENONP00			tr	h	1

IDS_JOYSTICK_IN_PORT_1		**	1	1

IDS_AUTOFIRE_SPEED			en	s	1
IDS_AUTOFIRE_SPEED			da	h	1
IDS_AUTOFIRE_SPEED			de	s	1
IDS_AUTOFIRE_SPEED			hu	s	2
IDS_AUTOFIRE_SPEED			it	V	1
IDS_AUTOFIRE_SPEED			nl	s	1
IDS_AUTOFIRE_SPEED			sv	H	1
IDS_AUTOFIRE_SPEED			tr	h	1

IDS_JOYSTICK_IN_PORT_2		**	2	1

IDS_JOY_CONFIG_A			**	A	1

IDS_JOY_CONFIG_B			**	B	1

IDS_JOY_CALIBRATE			en	C	1
IDS_JOY_CALIBRATE			da	K	1
IDS_JOY_CALIBRATE			de	k	2
IDS_JOY_CALIBRATE			fr	C	1
IDS_JOY_CALIBRATE			hu	k	3
IDS_JOY_CALIBRATE			it	C	1
IDS_JOY_CALIBRATE			nl	K	1
IDS_JOY_CALIBRATE			sv	K	1
IDS_JOY_CALIBRATE			tr	c	1

IDS_JOYSTICK_IN_EXTRA_PORT_1	**	1	1

IDS_JOYSTICK_IN_EXTRA_PORT_2	**	2	1

IDS_KEYSET_SW				en	o	1
IDS_KEYSET_SW				da	y	1
IDS_KEYSET_SW				fr	d	1
IDS_KEYSET_SW				hu	y	1
IDS_KEYSET_SW				it	u	1
IDS_KEYSET_SW				nl	u	1
IDS_KEYSET_SW				sv	y	1
IDS_KEYSET_SW				tr	n	1

IDS_KEYSET_S				**	S	1
IDS_KEYSET_S				hu	D	1
IDS_KEYSET_S				nl	Z	1
IDS_KEYSET_S				tr	y	1

IDS_KEYSET_SE				en	u	1
IDS_KEYSET_SE				da	d	1
IDS_KEYSET_SE				fr	u	1
IDS_KEYSET_SE				hu	l	2
IDS_KEYSET_SE				it	d	1
IDS_KEYSET_SE				nl	i	1
IDS_KEYSET_SE				sv	d	1
IDS_KEYSET_SE				tr	u	1

IDS_KEYSET_W				en	W	1
IDS_KEYSET_W				da	V	1
IDS_KEYSET_W				de	W	1
IDS_KEYSET_W				fr	O	1
IDS_KEYSET_W				hu	N	1
IDS_KEYSET_W				it	O	1
IDS_KEYSET_W				nl	W	1
IDS_KEYSET_W				sv	V	1
IDS_KEYSET_W				tr	B	1

IDS_KEYSET_E				en	E	1
IDS_KEYSET_E				da	Ø	1
IDS_KEYSET_E				de	O	1
IDS_KEYSET_E				fr	E	1
IDS_KEYSET_E				hu	K	1
IDS_KEYSET_E				it	E	1
IDS_KEYSET_E				nl	O	1
IDS_KEYSET_E				sv	Ö	1
IDS_KEYSET_E				tr	D	1

IDS_KEYSET_NW				en	r	1
IDS_KEYSET_NW				da	r	1
IDS_KEYSET_NW				fr	r	1
IDS_KEYSET_NW				hu	g	1
IDS_KEYSET_NW				it	r	1
IDS_KEYSET_NW				nl	r	1
IDS_KEYSET_NW				sv	r	1
IDS_KEYSET_NW				tr	z	1

IDS_KEYSET_N				**	N	1
IDS_KEYSET_N				hu	s	1
IDS_KEYSET_N				tr	K	1

IDS_KEYSET_NE				en	t	1
IDS_KEYSET_NE				da	o	1
IDS_KEYSET_NE				fr	o	1
IDS_KEYSET_NE				hu	e	1
IDS_KEYSET_NE				it	d	1
IDS_KEYSET_NE				nl	t	1
IDS_KEYSET_NE				sv	o	1
IDS_KEYSET_NE				tr	e	1

IDS_KEYSET_FIRE				en	F	1
IDS_KEYSET_FIRE				da	k	1
IDS_KEYSET_FIRE				de	F	1
IDS_KEYSET_FIRE				fr	B	1
IDS_KEYSET_FIRE				hu	T	1
IDS_KEYSET_FIRE				it	F	1
IDS_KEYSET_FIRE				nl	V	1
IDS_KEYSET_FIRE				sv	A	1
IDS_KEYSET_FIRE				tr	A	1

IDS_SOUND_SAMPLE_FREQUENCY		en	F	1
IDS_SOUND_SAMPLE_FREQUENCY		da	f	1
IDS_SOUND_SAMPLE_FREQUENCY		de	F	1
IDS_SOUND_SAMPLE_FREQUENCY		hu	f	1
IDS_SOUND_SAMPLE_FREQUENCY		it	F	1
IDS_SOUND_SAMPLE_FREQUENCY		nl	F	1
IDS_SOUND_SAMPLE_FREQUENCY		sv	f	1
IDS_SOUND_SAMPLE_FREQUENCY		tr	F	1

IDS_SOUND_BUFFER_SIZE			en	S	1
IDS_SOUND_BUFFER_SIZE			da	s	1
IDS_SOUND_BUFFER_SIZE			fr	t	1
IDS_SOUND_BUFFER_SIZE			hu	m	1
IDS_SOUND_BUFFER_SIZE			it	D	1
IDS_SOUND_BUFFER_SIZE			nl	g	1
IDS_SOUND_BUFFER_SIZE			sv	s	1
IDS_SOUND_BUFFER_SIZE			tr	S	1

IDS_SOUND_SYNCH_METHOD		en	M	1
IDS_SOUND_SYNCH_METHOD		da	m	1
IDS_SOUND_SYNCH_METHOD		de	m	1
IDS_SOUND_SYNCH_METHOD		fr	M	1
IDS_SOUND_SYNCH_METHOD		it	M	1
IDS_SOUND_SYNCH_METHOD		nl	m	1
IDS_SOUND_SYNCH_METHOD		sv	m	1
IDS_SOUND_SYNCH_METHOD		tr	M	1

IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	en	d	2
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	da	d	2
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	de	D	1
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	hu	m	2
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	it	d	1
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	nl	s	2
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	sv	d	2
IDS_TOGGLE_SNAPSHOT_SAVE_DISKS	tr	d	2

IDS_TOGGLE_SNAPSHOT_SAVE_ROMS	**	R	1

IDS_ROMSET_CONFIGURATION		en	C	1
IDS_ROMSET_CONFIGURATION		da	I	1
IDS_ROMSET_CONFIGURATION		de	K	1
IDS_ROMSET_CONFIGURATION		fr	C	1
IDS_ROMSET_CONFIGURATION		hu	K	1
IDS_ROMSET_CONFIGURATION		it	C	1
IDS_ROMSET_CONFIGURATION		nl	C	1
IDS_ROMSET_CONFIGURATION		sv	i	1
IDS_ROMSET_CONFIGURATION		tr	K	1

IDS_TOGGLE_CONSOLE_APPEND		en	A	1
IDS_TOGGLE_CONSOLE_APPEND		da	T	1
IDS_TOGGLE_CONSOLE_APPEND		de	a	2
IDS_TOGGLE_CONSOLE_APPEND		fr	A	1
IDS_TOGGLE_CONSOLE_APPEND		hu	a	1
IDS_TOGGLE_CONSOLE_APPEND		it	A	1
IDS_TOGGLE_CONSOLE_APPEND		nl	L	1
IDS_TOGGLE_CONSOLE_APPEND		sv	L	1
IDS_TOGGLE_CONSOLE_APPEND		tr	a	1

IDS_SYMBOLIC				**	S	1

IDS_POSITIONAL				**	P	1
IDS_POSITIONAL				tr	K	1

IDS_SYMBOLIC_US				**	S	1
IDS_SYMBOLIC_US				fr	U	1

IDS_SYMBOLIC_DE				**	S	1
IDS_SYMBOLIC_DE				en	y	1
IDS_SYMBOLIC_DE				fr	D	1

IDS_GR_SYM					**	G	1

IDS_GR_POS					**	r	1
IDS_GR_POS					fr	R	1

IDS_UK_SYM					**	U	1

IDS_UK_POS					**	K	1

IDS_DE_SYM					**	D	1
IDS_DE_SYM					it	T	1

IDS_DE_POS					**	E	1

IDS_A_MEMORY				en	M	1
IDS_A_MEMORY				da	H	1
IDS_A_MEMORY				de	S	1
IDS_A_MEMORY				fr	m	1
IDS_A_MEMORY				hu	M	1
IDS_A_MEMORY				it	M	1
IDS_A_MEMORY				nl	G	1
IDS_A_MEMORY				sv	M	1
IDS_A_MEMORY				tr	B	1

IDS_DRIVE_TYPE				en	D	1
IDS_DRIVE_TYPE				da	E	1
IDS_DRIVE_TYPE				de	G	1
IDS_DRIVE_TYPE				fr	l	1
IDS_DRIVE_TYPE				hu	L	1
IDS_DRIVE_TYPE				it	d	2
IDS_DRIVE_TYPE				nl	D	1
IDS_DRIVE_TYPE				sv	E	1
IDS_DRIVE_TYPE				tr	S	1

IDS_40_TRACK_HANDLING			en	t	1
IDS_40_TRACK_HANDLING			da	s	1
IDS_40_TRACK_HANDLING			de	S	1
IDS_40_TRACK_HANDLING			hu	s	1
IDS_40_TRACK_HANDLING			it	t	2
IDS_40_TRACK_HANDLING			nl	s	1
IDS_40_TRACK_HANDLING			sv	s	1
IDS_40_TRACK_HANDLING			tr	t	1

IDS_IDLE_METHOD				en	l	1
IDS_IDLE_METHOD				da	u	1
IDS_IDLE_METHOD				de	l	1
IDS_IDLE_METHOD				hu	j	1
IDS_IDLE_METHOD				it	l	1
IDS_IDLE_METHOD				nl	l	1
IDS_IDLE_METHOD				sv	u	1
IDS_IDLE_METHOD				tr	B	1

IDS_TOGGLE_DRIVE_PARALLEL_CABLE	**	P	1
IDS_TOGGLE_DRIVE_PARALLEL_CABLE	fr	p	1
IDS_TOGGLE_DRIVE_PARALLEL_CABLE	it	p	1

IDS_DRIVE_EXPANSION			en	e	2
IDS_DRIVE_EXPANSION			da	u	1
IDS_DRIVE_EXPANSION			de	E	1
IDS_DRIVE_EXPANSION			fr	E	1
IDS_DRIVE_EXPANSION			hu	b	1
IDS_DRIVE_EXPANSION			it	E	1
IDS_DRIVE_EXPANSION			nl	u	1
IDS_DRIVE_EXPANSION			sv	u	1
IDS_DRIVE_EXPANSION			tr	e	1

IDS_TOGGLE_DRIVE_EXPANSION_2000	**	R	1

IDS_TOGGLE_DRIVE_EXPANSION_4000	**	4	1

IDS_TOGGLE_DRIVE_EXPANSION_6000	**	6	1

IDS_TOGGLE_DRIVE_EXPANSION_8000	**	M	1

IDS_TOGGLE_DRIVE_EXPANSION_A000	**	A	1

IDS_PLUS4_VIC20_MEMORY		en	M	1
IDS_PLUS4_VIC20_MEMORY		da	H	1
IDS_PLUS4_VIC20_MEMORY		de	S	1
IDS_PLUS4_VIC20_MEMORY		fr	m	1
IDS_PLUS4_VIC20_MEMORY		hu	M	1
IDS_PLUS4_VIC20_MEMORY		it	M	1
IDS_PLUS4_VIC20_MEMORY		nl	G	1
IDS_PLUS4_VIC20_MEMORY		sv	M	1
IDS_PLUS4_VIC20_MEMORY		tr	B	1

IDS_MP_FILE				en	F	1
IDS_MP_FILE				da	F	1
IDS_MP_FILE				de	D	1
IDS_MP_FILE				fr	F	1
IDS_MP_FILE				hu	F	1
IDS_MP_FILE				it	F	1
IDS_MP_FILE				nl	B	1
IDS_MP_FILE				sv	A	1
IDS_MP_FILE				tr	D	1

IDS_MP_ATTACH_DISK_IMAGE		en	d	1
IDS_MP_ATTACH_DISK_IMAGE		da	D	1
IDS_MP_ATTACH_DISK_IMAGE		de	D	1
IDS_MP_ATTACH_DISK_IMAGE		fr	d	2
IDS_MP_ATTACH_DISK_IMAGE		it	d	1
IDS_MP_ATTACH_DISK_IMAGE		nl	s	1
IDS_MP_ATTACH_DISK_IMAGE		sv	d	1
IDS_MP_DETACH_DISK_IMAGE		sv	f	1
IDS_MP_ATTACH_DISK_IMAGE		tr	D	1

IDS_MP_DETACH_DISK_IMAGE		en	e	1
IDS_MP_DETACH_DISK_IMAGE		da	F	1
IDS_MP_DETACH_DISK_IMAGE		de	e	2
IDS_MP_DETACH_DISK_IMAGE		fr	R	1
IDS_MP_DETACH_DISK_IMAGE		hu	l	1
IDS_MP_DETACH_DISK_IMAGE		it	R	1
IDS_MP_DETACH_DISK_IMAGE		nl	e	1
IDS_MP_DETACH_DISK_IMAGE		tr	t	1

IDS_MP_FLIP_LIST			en	F	1
IDS_MP_FLIP_LIST			da	B	1
IDS_MP_FLIP_LIST			de	F	1
IDS_MP_FLIP_LIST			fr	G	1
IDS_MP_FLIP_LIST			hu	i	1
IDS_MP_FLIP_LIST			it	F	1
IDS_MP_FLIP_LIST			nl	F	1
IDS_MP_FLIP_LIST			sv	V	1
IDS_MP_FLIP_LIST			tr	S	1

IDS_MP_DATASETTE_CONTROL		en	l	1
IDS_MP_DATASETTE_CONTROL		da	l	1
IDS_MP_DATASETTE_CONTROL		de	l	2
IDS_MP_DATASETTE_CONTROL		fr	l	1
IDS_MP_DATASETTE_CONTROL		hu	v	1
IDS_MP_DATASETTE_CONTROL		it	l	1
IDS_MP_DATASETTE_CONTROL		nl	n	1
IDS_MP_DATASETTE_CONTROL		sv	s	2
IDS_MP_DATASETTE_CONTROL		tr	l	1

IDS_MP_ATTACH_CARTRIDGE_IMAGE	en	c	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	da	c	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	de	m	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	it	c	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	nl	c	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	sv	i	1
IDS_MP_ATTACH_CARTRIDGE_IMAGE	tr	K	1

IDS_MP_RESET				**	R	1
IDS_MP_RESET				hu	r	1
IDS_MP_RESET				sv	N	1

IDS_MP_DEBUG				**	D	1
IDS_MP_DEBUG				hu	N	1
IDS_MP_DEBUG				sv	F	1

IDS_MP_MODE				en	o	1
IDS_MP_MODE				da	T	1
IDS_MP_MODE				de	o	1
IDS_MP_MODE				fr	M	1
IDS_MP_MODE				hu	d	1
IDS_MP_MODE				it	o	1
IDS_MP_MODE				sv	L	1
IDS_MP_MODE				tr	o	1

IDS_MP_SNAPSHOT				en	p	1
IDS_MP_SNAPSHOT				da	p	1
IDS_MP_SNAPSHOT				de	p	1
IDS_MP_SNAPSHOT				fr	S	1
IDS_MP_SNAPSHOT				hu	P	1
IDS_MP_SNAPSHOT				it	p	1
IDS_MP_SNAPSHOT				nl	p	1
IDS_MP_SNAPSHOT				sv	Ö	1
IDS_MP_SNAPSHOT				tr	A	1

IDS_MP_OPTIONS				**	O	1
IDS_MP_OPTIONS				da	I	1
IDS_MP_OPTIONS				sv	A	1
IDS_MP_OPTIONS				tr	S	1

IDS_MP_REFRESH_RATE			en	R	1
IDS_MP_REFRESH_RATE			da	O	1
IDS_MP_REFRESH_RATE			de	r	1
IDS_MP_REFRESH_RATE			fr	r	1
IDS_MP_REFRESH_RATE			hu	r	2
IDS_MP_REFRESH_RATE			it	a	2
IDS_MP_REFRESH_RATE			nl	r	1
IDS_MP_REFRESH_RATE			sv	U	1
IDS_MP_REFRESH_RATE			tr	Y	1

IDS_MP_MAXIMUM_SPEED			**	M	1
IDS_MP_MAXIMUM_SPEED			it	m	1

IDS_MP_VIDEO_STANDARD			en	o	1
IDS_MP_VIDEO_STANDARD			da	T	1
IDS_MP_VIDEO_STANDARD			de	o	1
IDS_MP_VIDEO_STANDARD			fr	d	2
IDS_MP_VIDEO_STANDARD			hu	s	1
IDS_MP_VIDEO_STANDARD			it	o	1
IDS_MP_VIDEO_STANDARD			nl	o	1
IDS_MP_VIDEO_STANDARD			sv	T	1
IDS_MP_VIDEO_STANDARD			tr	o	1

IDS_MP_DRIVE_SYNC_FACTOR		**	y	1
IDS_MP_DRIVE_SYNC_FACTOR		hu	i	1
IDS_MP_DRIVE_SYNC_FACTOR		it	i	2

IDS_MP_SETTINGS				en	e	1
IDS_MP_SETTINGS				da	I	1
IDS_MP_SETTINGS				de	E	1
IDS_MP_SETTINGS				fr	P	1
IDS_MP_SETTINGS				hu	e	1
IDS_MP_SETTINGS				it	m	1
IDS_MP_SETTINGS				nl	e	1
IDS_MP_SETTINGS				sv	I	1
IDS_MP_SETTINGS				tr	A	1

IDS_MP_CARTRIDGE_IO_SETTINGS	en	C	1
IDS_MP_CARTRIDGE_IO_SETTINGS	da	C	1
IDS_MP_CARTRIDGE_IO_SETTINGS	fr	c	1
IDS_MP_CARTRIDGE_IO_SETTINGS	hu	C	1
IDS_MP_CARTRIDGE_IO_SETTINGS	it	c	1
IDS_MP_CARTRIDGE_IO_SETTINGS	nl	C	1
IDS_MP_CARTRIDGE_IO_SETTINGS	sv	M	1
IDS_MP_CARTRIDGE_IO_SETTINGS	tr	K	1

IDS_MP_LANGUAGE				en	L	1
IDS_MP_LANGUAGE				da	S	1
IDS_MP_LANGUAGE				fr	L	1
IDS_MP_LANGUAGE				hu	N	1
IDS_MP_LANGUAGE				it	L	1
IDS_MP_LANGUAGE				nl	T	1
IDS_MP_LANGUAGE				sv	S	1
IDS_MP_LANGUAGE				tr	l	1

IDS_MP_HELP				en	H	1
IDS_MP_HELP				da	H	1
IDS_MP_HELP				de	H	1
IDS_MP_HELP				fr	A	1
IDS_MP_HELP				hu	S	1
IDS_MP_HELP				it	A	1
IDS_MP_HELP				nl	H	1
IDS_MP_HELP				sv	H	1
IDS_MP_HELP				tr	Y	1

IDS_MP_VIEW				en	V	1
IDS_MP_VIEW				da	V	1
IDS_MP_VIEW				de	s	1
IDS_MP_VIEW				fr	A	1
IDS_MP_VIEW				hu	N	1
IDS_MP_VIEW				it	V	1
IDS_MP_VIEW				nl	B	1
IDS_MP_VIEW				sv	V	1
IDS_MP_VIEW				tr	G	1

IDS_MP_WINDOW				en	W	1
IDS_MP_WINDOW				da	n	1
IDS_MP_WINDOW				de	F	1
IDS_MP_WINDOW				fr	F	1
IDS_MP_WINDOW				hu	A	1
IDS_MP_WINDOW				it	n	1
IDS_MP_WINDOW				nl	V	1
IDS_MP_WINDOW				sv	F	1
IDS_MP_WINDOW				tr	P	1

IDS_MI_EXIT				en	x	1
IDS_MI_EXIT				da	s	1
IDS_MI_EXIT				de	x	1
IDS_MI_EXIT				fr	x	1
IDS_MI_EXIT				hu	K	1
IDS_MI_EXIT				it	E	1
IDS_MI_EXIT				nl	A	1
IDS_MI_EXIT				sv	A	1
IDS_MI_EXIT				tr	k	1

IDS_MI_ABOUT				en	A	1
IDS_MI_ABOUT				da	O	1
IDS_MI_ABOUT				de	Ü	1
IDS_MI_ABOUT				fr	P	1
IDS_MI_ABOUT				hu	N	1
IDS_MI_ABOUT				it	I	1
IDS_MI_ABOUT				nl	O	1
IDS_MI_ABOUT				sv	O	1
IDS_MI_ABOUT				tr	a	1

IDS_MI_PAUSE				**	P	1
IDS_MI_PAUSE				hu	S	1
IDS_MI_PAUSE				tr	D	1

IDS_MI_EDIT_COPY			en	C	1
IDS_MI_EDIT_COPY			da	K	1
IDS_MI_EDIT_COPY			de	K	1
IDS_MI_EDIT_COPY			hu	M	1
IDS_MI_EDIT_COPY			it	C	1
IDS_MI_EDIT_COPY			nl	C	1
IDS_MI_EDIT_COPY			sv	K	1
IDS_MI_EDIT_COPY			tr	K	1

IDS_MI_EDIT_PASTE			en	P	1
IDS_MI_EDIT_PASTE			da	I	1
IDS_MI_EDIT_PASTE			de	E	1
IDS_MI_EDIT_PASTE			hu	B	1
IDS_MI_EDIT_PASTE			it	I	1
IDS_MI_EDIT_PASTE			nl	P	1
IDS_MI_EDIT_PASTE			sv	l	1
IDS_MI_EDIT_PASTE			tr	p	1

IDS_MI_AUTOSTART			**	A	1
IDS_MI_AUTOSTART			fr	a	3
IDS_MI_AUTOSTART			hu	a	3
IDS_MI_AUTOSTART			tr	a	3

IDS_MI_RESET_HARD			**	H	1

IDS_MI_RESET_SOFT			en	S	1
IDS_MI_RESET_SOFT			da	B	1
IDS_MI_RESET_SOFT			de	W	1
IDS_MI_RESET_SOFT			hu	M	1
IDS_MI_RESET_SOFT			it	S	1
IDS_MI_RESET_SOFT			nl	Z	1
IDS_MI_RESET_SOFT			sv	M	1
IDS_MI_RESET_SOFT			tr	S	1

IDS_MI_DRIVE8				**	8	1

IDS_MI_DRIVE9				**	9	1

IDS_MI_DRIVE10				**	0	1

IDS_MI_DRIVE11				**	1	2

IDS_MI_ATTACH_TAPE			en	t	3
IDS_MI_ATTACH_TAPE			da	T	1
IDS_MI_ATTACH_TAPE			de	B	1
IDS_MI_ATTACH_TAPE			hu	S	1
IDS_MI_ATTACH_TAPE			it	c	1
IDS_MI_ATTACH_TAPE			nl	t	1
IDS_MI_ATTACH_TAPE			sv	b	1
IDS_MI_ATTACH_TAPE			tr	T	1

IDS_MI_DETACH_TAPE			en	h	1
IDS_MI_DETACH_TAPE			da	r	1
IDS_MI_DETACH_TAPE			fr	r	1
IDS_MI_DETACH_TAPE			hu	a	1
IDS_MI_DETACH_TAPE			it	v	1
IDS_MI_DETACH_TAPE			nl	l	1
IDS_MI_DETACH_TAPE			sv	r	1
IDS_MI_DETACH_TAPE			tr	k	1

IDS_MI_DETACH_ALL			en	A	1
IDS_MI_DETACH_ALL			da	A	1
IDS_MI_DETACH_ALL			de	A	1
IDS_MI_DETACH_ALL			hu	M	1
IDS_MI_DETACH_ALL			it	T	1
IDS_MI_DETACH_ALL			nl	A	1
IDS_MI_DETACH_ALL			sv	A	1
IDS_MI_DETACH_ALL			tr	T	1

IDS_MI_TOGGLE_SOUND			en	S	1
IDS_MI_TOGGLE_SOUND			da	y	1
IDS_MI_TOGGLE_SOUND			de	S	1
IDS_MI_TOGGLE_SOUND			fr	a	1
IDS_MI_TOGGLE_SOUND			hu	H	1
IDS_MI_TOGGLE_SOUND			it	a	1
IDS_MI_TOGGLE_SOUND			nl	G	1
IDS_MI_TOGGLE_SOUND			sv	l	1
IDS_MI_TOGGLE_SOUND			tr	S	1

IDS_MI_TOGGLE_DOUBLESIZE		**	D	1
IDS_MI_TOGGLE_DOUBLESIZE		fr	T	1
IDS_MI_TOGGLE_DOUBLESIZE		tr	b	1
IDS_MI_TOGGLE_DOUBLESCAN		tr	t	2

IDS_MI_TOGGLE_DOUBLESCAN		en	b	1
IDS_MI_TOGGLE_DOUBLESCAN		da	b	1
IDS_MI_TOGGLE_DOUBLESCAN		de	p	1
IDS_MI_TOGGLE_DOUBLESCAN		hu	p	1
IDS_MI_TOGGLE_DOUBLESCAN		it	p	1
IDS_MI_TOGGLE_DOUBLESCAN		nl	b	1
IDS_MI_TOGGLE_DOUBLESCAN		sv	b	1

IDS_MI_DRIVE_TRUE_EMULATION	en	T	1
IDS_MI_DRIVE_TRUE_EMULATION	da	t	1
IDS_MI_DRIVE_TRUE_EMULATION	de	P	1
IDS_MI_DRIVE_TRUE_EMULATION	fr	r	2
IDS_MI_DRIVE_TRUE_EMULATION	hu	I	1
IDS_MI_DRIVE_TRUE_EMULATION	it	h	1
IDS_MI_DRIVE_TRUE_EMULATION	nl	H	1
IDS_MI_DRIVE_TRUE_EMULATION	sv	Ä	1
IDS_MI_DRIVE_TRUE_EMULATION	tr	G	1

IDS_MI_AUTOSTART_HANDLE_TDE	**	n	1
IDS_MI_AUTOSTART_HANDLE_TDE	tr	n	2

IDS_MI_TOGGLE_VIDEOCACHE		**	c	1
IDS_MI_TOGGLE_VIDEOCACHE		fr	C	1
IDS_MI_TOGGLE_VIDEOCACHE		it	C	1
IDS_MI_TOGGLE_VIDEOCACHE		tr	n	2

IDS_MI_DRIVE_SETTINGS			en	D	1
IDS_MI_DRIVE_SETTINGS			da	D	1
IDS_MI_DRIVE_SETTINGS			de	F	1
IDS_MI_DRIVE_SETTINGS			hu	L	1
IDS_MI_DRIVE_SETTINGS			it	d	1
IDS_MI_DRIVE_SETTINGS			nl	D	1
IDS_MI_DRIVE_SETTINGS			sv	D	1
IDS_MI_DRIVE_SETTINGS			tr	S	1

IDS_MI_CART_ATTACH_CRT		**	C	1

IDS_MI_CART_ATTACH_8KB		**	8	1

IDS_MI_CART_ATTACH_16KB		**	1	1

IDS_MI_CART_ATTACH_AR			**	A	1

IDS_MI_CART_ATTACH_AR3		**	3	1

IDS_MI_CART_ATTACH_AR4		**	4	1

IDS_MI_CART_ATTACH_STARDOS		**	S	1

IDS_MI_CART_ATTACH_AT			**	P	1

IDS_MI_CART_ATTACH_EPYX		**	E	1

IDS_MI_CART_ATTACH_IEEE488		**	I	1
IDS_MI_CART_ATTACH_IEEE488		it	I	2

IDS_MI_CART_ATTACH_RR			**	R	1

IDS_MI_CART_ATTACH_MMC_REPLAY	**	M	1

IDS_MI_CART_ATTACH_IDE64		**	6	1

IDS_MI_CART_ATTACH_SS4		**	u	1

IDS_MI_CART_ATTACH_SS5		**	5	1

IDS_MI_CART_ATTACH_STB		**	B	1

IDS_MI_FLIP_ADD				en	A	1
IDS_MI_FLIP_ADD				da	T	1
IDS_MI_FLIP_ADD				de	A	1
IDS_MI_FLIP_ADD				hu	a	1
IDS_MI_FLIP_ADD				it	A	1
IDS_MI_FLIP_ADD				nl	V	1
IDS_MI_FLIP_ADD				sv	L	1
IDS_MI_FLIP_ADD				tr	a	1

IDS_MI_FLIP_REMOVE			en	R	1
IDS_MI_FLIP_REMOVE			da	F	1
IDS_MI_FLIP_REMOVE			de	r	1
IDS_MI_FLIP_REMOVE			hu	e	1
IDS_MI_FLIP_REMOVE			it	R	1
IDS_MI_FLIP_REMOVE			nl	w	1
IDS_MI_FLIP_REMOVE			sv	T	1
IDS_MI_FLIP_REMOVE			tr	r	2

IDS_MI_FLIP_NEXT			en	n	1
IDS_MI_FLIP_NEXT			da	n	1
IDS_MI_FLIP_NEXT			de	N	1
IDS_MI_FLIP_NEXT			hu	K	1
IDS_MI_FLIP_NEXT			it	s	1
IDS_MI_FLIP_NEXT			nl	K	1
IDS_MI_FLIP_NEXT			sv	n	2
IDS_MI_FLIP_NEXT			tr	n	1

IDS_MI_FLIP_PREVIOUS			en	p	1
IDS_MI_FLIP_PREVIOUS			da	o	1
IDS_MI_FLIP_PREVIOUS			de	V	1
IDS_MI_FLIP_PREVIOUS			hu	E	1
IDS_MI_FLIP_PREVIOUS			it	p	1
IDS_MI_FLIP_PREVIOUS			nl	o	1
IDS_MI_FLIP_PREVIOUS			sv	f	1
IDS_MI_FLIP_PREVIOUS			tr	k	1

IDS_MI_FLIP_LOAD			en	L	1
IDS_MI_FLIP_LOAD			da	l	1
IDS_MI_FLIP_LOAD			de	L	1
IDS_MI_FLIP_LOAD			fr	C	1
IDS_MI_FLIP_LOAD			hu	L	1
IDS_MI_FLIP_LOAD			it	C	1
IDS_MI_FLIP_LOAD			nl	L	1
IDS_MI_FLIP_LOAD			sv	L	1
IDS_MI_FLIP_LOAD			tr	l	2

IDS_MI_FLIP_SAVE			en	S	1
IDS_MI_FLIP_SAVE			da	s	1
IDS_MI_FLIP_SAVE			de	S	1
IDS_MI_FLIP_SAVE			fr	E	1
IDS_MI_FLIP_SAVE			hu	s	2
IDS_MI_FLIP_SAVE			it	S	1
IDS_MI_FLIP_SAVE			nl	s	1
IDS_MI_FLIP_SAVE			sv	S	1
IDS_MI_FLIP_SAVE			tr	S	1

IDS_MI_DATASETTE_STOP			**	t	1
IDS_MI_DATASETTE_STOP			fr	A	1
IDS_MI_DATASETTE_STOP			hu	L	1
IDS_MI_DATASETTE_STOP			tr	D	1

IDS_MI_DATASETTE_START		**	S	1
IDS_MI_DATASETTE_START		fr	D	1
IDS_MI_DATASETTE_START		hu	I	1
IDS_MI_DATASETTE_START		it	A	1

IDS_MI_DATASETTE_FORWARD		en	F	1
IDS_MI_DATASETTE_FORWARD		da	f	1
IDS_MI_DATASETTE_FORWARD		de	F	1
IDS_MI_DATASETTE_FORWARD		fr	a	1
IDS_MI_DATASETTE_FORWARD		hu	E	1
IDS_MI_DATASETTE_FORWARD		it	A	1
IDS_MI_DATASETTE_FORWARD		nl	V	1
IDS_MI_DATASETTE_FORWARD		sv	f	1
IDS_MI_DATASETTE_FORWARD		tr	r	1

IDS_MI_DATASETTE_REWIND		en	R	1
IDS_MI_DATASETTE_REWIND		da	b	1
IDS_MI_DATASETTE_REWIND		de	R	1
IDS_MI_DATASETTE_REWIND		fr	r	1
IDS_MI_DATASETTE_REWIND		hu	V	1
IDS_MI_DATASETTE_REWIND		it	I	1
IDS_MI_DATASETTE_REWIND		nl	r	1
IDS_MI_DATASETTE_REWIND		sv	b	1
IDS_MI_DATASETTE_REWIND		tr	G	1

IDS_MI_DATASETTE_RECORD		en	c	1
IDS_MI_DATASETTE_RECORD		da	O	1
IDS_MI_DATASETTE_RECORD		de	c	1
IDS_MI_DATASETTE_RECORD		fr	g	1
IDS_MI_DATASETTE_RECORD		it	c	1
IDS_MI_DATASETTE_RECORD		nl	n	1
IDS_MI_DATASETTE_RECORD		sv	i	1
IDS_MI_DATASETTE_RECORD		tr	K	1

IDS_MI_DATASETTE_RESET		**	e	1
IDS_MI_DATASETTE_RESET		hu	l	1
IDS_MI_DATASETTE_RESET		sv	N	1

IDS_MI_DATASETTE_RESET_COUNTER	en	o	1
IDS_MI_DATASETTE_RESET_COUNTER	da	æ	1
IDS_MI_DATASETTE_RESET_COUNTER	de	ä	1
IDS_MI_DATASETTE_RESET_COUNTER	fr	o	1
IDS_MI_DATASETTE_RESET_COUNTER	hu	n	1
IDS_MI_DATASETTE_RESET_COUNTER	it	o	1
IDS_MI_DATASETTE_RESET_COUNTER	nl	e	3
IDS_MI_DATASETTE_RESET_COUNTER	sv	ä	2
IDS_MI_DATASETTE_RESET_COUNTER	tr	R	1

IDS_MI_CART_SET_DEFAULT		en	d	2
IDS_MI_CART_SET_DEFAULT		da	d	2
IDS_MI_CART_SET_DEFAULT		de	d	2
IDS_MI_CART_SET_DEFAULT		fr	d	1
IDS_MI_CART_SET_DEFAULT		hu	a	2
IDS_MI_CART_SET_DEFAULT		it	p	2
IDS_MI_CART_SET_DEFAULT		nl	d	2
IDS_MI_CART_SET_DEFAULT		sv	f	1
IDS_MI_CART_SET_DEFAULT		tr	v	1

IDS_MI_TOGGLE_CART_RESET		en	o	1
IDS_MI_TOGGLE_CART_RESET		da	v	1
IDS_MI_TOGGLE_CART_RESET		fr	h	1
IDS_MI_TOGGLE_CART_RESET		hu	c	2
IDS_MI_TOGGLE_CART_RESET		it	a	1
IDS_MI_TOGGLE_CART_RESET		nl	l	1
IDS_MI_TOGGLE_CART_RESET		sv	v	1
IDS_MI_TOGGLE_CART_RESET		tr	d	1

IDS_MI_CART_DETACH			en	i	2
IDS_MI_CART_DETACH			da	i	2
IDS_MI_CART_DETACH			de	I	1
IDS_MI_CART_DETACH			fr	o	1
IDS_MI_CART_DETACH			hu	l	1
IDS_MI_CART_DETACH			it	i	3
IDS_MI_CART_DETACH			nl	i	1
IDS_MI_CART_DETACH			sv	f	1
IDS_MI_CART_DETACH			tr	i	1

IDS_MI_CART_FREEZE			en	z	1
IDS_MI_CART_FREEZE			da	f	1
IDS_MI_CART_FREEZE			de	z	1
IDS_MI_CART_FREEZE			hu	F	1
IDS_MI_CART_FREEZE			it	z	1
IDS_MI_CART_FREEZE			nl	z	1
IDS_MI_CART_FREEZE			sv	f	1
IDS_MI_CART_FREEZE			tr	K	1

IDS_MI_MONITOR				**	M	1

IDS_MI_DEBUG_MODE_NORMAL		**	N	1

IDS_MI_DEBUG_MODE_SMALL		en	S	1
IDS_MI_DEBUG_MODE_SMALL		da	L	1
IDS_MI_DEBUG_MODE_SMALL		de	K	1
IDS_MI_DEBUG_MODE_SMALL		fr	P	1
IDS_MI_DEBUG_MODE_SMALL		hu	K	1
IDS_MI_DEBUG_MODE_SMALL		it	P	1
IDS_MI_DEBUG_MODE_SMALL		nl	K	1
IDS_MI_DEBUG_MODE_SMALL		sv	L	1
IDS_MI_DEBUG_MODE_SMALL		tr	K	1

IDS_MI_DEBUG_MODE_HISTORY		en	H	1
IDS_MI_DEBUG_MODE_HISTORY		da	H	1
IDS_MI_DEBUG_MODE_HISTORY		de	H	1
IDS_MI_DEBUG_MODE_HISTORY		fr	H	1
IDS_MI_DEBUG_MODE_HISTORY		hu	E	1
IDS_MI_DEBUG_MODE_HISTORY		it	C	1
IDS_MI_DEBUG_MODE_HISTORY		nl	G	1
IDS_MI_DEBUG_MODE_HISTORY		sv	H	1
IDS_MI_DEBUG_MODE_HISTORY		tr	h	1

IDS_MI_DEBUG_MODE_AUTOPLAY		en	A	1
IDS_MI_DEBUG_MODE_AUTOPLAY		da	H	1
IDS_MI_DEBUG_MODE_AUTOPLAY		de	H	1
IDS_MI_DEBUG_MODE_AUTOPLAY		fr	i	1
IDS_MI_DEBUG_MODE_AUTOPLAY		hu	l	1
IDS_MI_DEBUG_MODE_AUTOPLAY		it	C	1
IDS_MI_DEBUG_MODE_AUTOPLAY		nl	A	1
IDS_MI_DEBUG_MODE_AUTOPLAY		sv	S	1
IDS_MI_DEBUG_MODE_AUTOPLAY		tr	h	1

IDS_MI_TOGGLE_MAINCPU_TRACE	en	M	1
IDS_MI_TOGGLE_MAINCPU_TRACE	da	C	1
IDS_MI_TOGGLE_MAINCPU_TRACE	de	H	1
IDS_MI_TOGGLE_MAINCPU_TRACE	hu	F	1
IDS_MI_TOGGLE_MAINCPU_TRACE	it	p	1
IDS_MI_TOGGLE_MAINCPU_TRACE	nl	H	1
IDS_MI_TOGGLE_MAINCPU_TRACE	sv	h	1
IDS_MI_TOGGLE_MAINCPU_TRACE	tr	m	1

IDS_MI_TOGGLE_DRIVE0CPU_TRACE	**	0	1

IDS_MI_TOGGLE_DRIVE1CPU_TRACE	**	1	1

IDS_MI_SNAPSHOT_LOAD			en	i	1
IDS_MI_SNAPSHOT_LOAD			da	I	1
IDS_MI_SNAPSHOT_LOAD			de	I	1
IDS_MI_SNAPSHOT_LOAD			fr	h	1
IDS_MI_SNAPSHOT_LOAD			hu	b	1
IDS_MI_SNAPSHOT_LOAD			it	i	2
IDS_MI_SNAPSHOT_LOAD			nl	a	4
IDS_MI_SNAPSHOT_LOAD			sv	L	1

IDS_MI_SNAPSHOT_SAVE			en	p	1
IDS_MI_SNAPSHOT_SAVE			da	p	1
IDS_MI_SNAPSHOT_SAVE			de	p	1
IDS_MI_SNAPSHOT_SAVE			hu	m	1
IDS_MI_SNAPSHOT_SAVE			it	p	1
IDS_MI_SNAPSHOT_SAVE			nl	p	2
IDS_MI_SNAPSHOT_SAVE			sv	ö	1
IDS_MI_SNAPSHOT_SAVE			tr	k	2

IDS_MI_LOADQUICK			en	L	1
IDS_MI_LOADQUICK			da	l	1
IDS_MI_LOADQUICK			de	l	1
IDS_MI_LOADQUICK			hu	b	1
IDS_MI_LOADQUICK			it	C	1
IDS_MI_LOADQUICK			nl	l	1
IDS_MI_LOADQUICK			sv	Ö	1
IDS_MI_LOADQUICK			tr	l	3

IDS_MI_SAVEQUICK			en	S	1
IDS_MI_SAVEQUICK			da	s	1
IDS_MI_SAVEQUICK			de	s	1
IDS_MI_SAVEQUICK			hu	m	1
IDS_MI_SAVEQUICK			it	S	1
IDS_MI_SAVEQUICK			nl	S	1
IDS_MI_SAVEQUICK			sv	S	1
IDS_MI_SAVEQUICK			tr	y	1

IDS_MI_EVENT_TOGGLE_RECORD		en	R	1
IDS_MI_EVENT_TOGGLE_RECORD		da	h	1
IDS_MI_EVENT_TOGGLE_RECORD		de	r	1
IDS_MI_EVENT_TOGGLE_RECORD		fr	g	1
IDS_MI_EVENT_TOGGLE_RECORD		hu	f	1
IDS_MI_EVENT_TOGGLE_RECORD		it	r	2
IDS_MI_EVENT_TOGGLE_RECORD		nl	r	1
IDS_MI_EVENT_TOGGLE_RECORD		sv	h	1
IDS_MI_EVENT_TOGGLE_RECORD		tr	r	2

IDS_MI_EVENT_TOGGLE_PLAYBACK	en	a	2
IDS_MI_EVENT_TOGGLE_PLAYBACK	da	h	1
IDS_MI_EVENT_TOGGLE_PLAYBACK	de	a	1
IDS_MI_EVENT_TOGGLE_PLAYBACK	fr	l	3
IDS_MI_EVENT_TOGGLE_PLAYBACK	hu	v	1
IDS_MI_EVENT_TOGGLE_PLAYBACK	it	i	3
IDS_MI_EVENT_TOGGLE_PLAYBACK	nl	A	1
IDS_MI_EVENT_TOGGLE_PLAYBACK	sv	u	2

IDS_MI_EVENT_START_MODE_SAVE	en	S	1
IDS_MI_EVENT_START_MODE_SAVE	da	s	1
IDS_MI_EVENT_START_MODE_SAVE	de	S	1
IDS_MI_EVENT_START_MODE_SAVE	fr	E	1
IDS_MI_EVENT_START_MODE_SAVE	hu	m	1
IDS_MI_EVENT_START_MODE_SAVE	it	S	1
IDS_MI_EVENT_START_MODE_SAVE	nl	s	1
IDS_MI_EVENT_START_MODE_SAVE	sv	S	1
IDS_MI_EVENT_START_MODE_SAVE	tr	k	2

IDS_MI_EVENT_START_MODE_LOAD	en	L	1
IDS_MI_EVENT_START_MODE_LOAD	da	l	1
IDS_MI_EVENT_START_MODE_LOAD	de	L	1
IDS_MI_EVENT_START_MODE_LOAD	fr	C	1
IDS_MI_EVENT_START_MODE_LOAD	hu	b	1
IDS_MI_EVENT_START_MODE_LOAD	it	C	1
IDS_MI_EVENT_START_MODE_LOAD	nl	L	1
IDS_MI_EVENT_START_MODE_LOAD	sv	L	1
IDS_MI_EVENT_START_MODE_LOAD	tr	l	2

IDS_MI_EVENT_START_MODE_RESET	en	r	2
IDS_MI_EVENT_START_MODE_RESET	da	r	2
IDS_MI_EVENT_START_MODE_RESET	de	R	1
IDS_MI_EVENT_START_MODE_RESET	fr	R	1
IDS_MI_EVENT_START_MODE_RESET	hu	R	1
IDS_MI_EVENT_START_MODE_RESET	it	r	1
IDS_MI_EVENT_START_MODE_RESET	nl	r	2
IDS_MI_EVENT_START_MODE_RESET	sv	n	1
IDS_MI_EVENT_START_MODE_RESET	tr	R	1

IDS_MI_EVENT_START_MODE_PLAYBCK	en	P	1
IDS_MI_EVENT_START_MODE_PLAYBCK	da	p	1
IDS_MI_EVENT_START_MODE_PLAYBCK	fr	c	1
IDS_MI_EVENT_START_MODE_PLAYBCK	hu	f	1
IDS_MI_EVENT_START_MODE_PLAYBCK	it	r	3
IDS_MI_EVENT_START_MODE_PLAYBCK	nl	g	1
IDS_MI_EVENT_START_MODE_PLAYBCK	sv	ö	1
IDS_MI_EVENT_START_MODE_PLAYBCK	tr	z	1

IDS_MI_REFRESH_RATE_AUTO		**	A	1
IDS_MI_REFRESH_RATE_AUTO		tr	a	1

IDS_MI_MAXIMUM_SPEED_NO_LIMIT	en	l	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	da	U	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	de	L	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	fr	l	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	hu	h	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	it	l	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	nl	l	1
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	sv	g	2
IDS_MI_MAXIMUM_SPEED_NO_LIMIT	tr	L	1

IDS_MI_MAXIMUM_SPEED_CUSTOM	en	C	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	da	E	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	de	B	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	fr	P	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	hu	E	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	it	P	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	nl	A	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	sv	E	1
IDS_MI_MAXIMUM_SPEED_CUSTOM	tr	e	1

IDS_MI_TOGGLE_WARP_MODE		**	W	1
IDS_MI_TOGGLE_WARP_MODE		hu	H	1
IDS_MI_TOGGLE_WARP_MODE		it	t	2

IDS_MI_SWAP_JOYSTICK			en	J	1
IDS_MI_SWAP_JOYSTICK			da	j	1
IDS_MI_SWAP_JOYSTICK			de	J	1
IDS_MI_SWAP_JOYSTICK			hu	f	1
IDS_MI_SWAP_JOYSTICK			it	J	1
IDS_MI_SWAP_JOYSTICK			nl	J	1
IDS_MI_SWAP_JOYSTICK			sv	s	1
IDS_MI_SWAP_JOYSTICK			tr	J	1

IDS_MI_SWAP_EXTRA_JOYSTICK		**	U	1
IDS_MI_SWAP_EXTRA_JOYSTICK		da	u	1
IDS_MI_SWAP_EXTRA_JOYSTICK		sv	a	2

IDS_MI_TOGGLE_VIRTUAL_DEVICES	**	V	1
IDS_MI_TOGGLE_VIRTUAL_DEVICES	fr	v	2
IDS_MI_TOGGLE_VIRTUAL_DEVICES	it	v	2
IDS_MI_TOGGLE_VIRTUAL_DEVICES	tr	y	1

IDS_MI_MOUSE				en	G	1
IDS_MI_MOUSE				da	g	1
IDS_MI_MOUSE				it	C	1
IDS_MI_MOUSE				nl	P	1
IDS_MI_MOUSE				sv	F	1
IDS_MI_MOUSE				tr	y	2

IDS_MI_C64MODEL_SETTINGS		**	C	1

IDS_MI_AUTOSTART_SETTINGS		**	A	1
IDS_MI_AUTOSTART_SETTINGS		tr	a	1

IDS_MI_VIDEO_SETTINGS			en	V	1
IDS_MI_VIDEO_SETTINGS			da	G	1
IDS_MI_VIDEO_SETTINGS			de	V	1
IDS_MI_VIDEO_SETTINGS			hu	V	1
IDS_MI_VIDEO_SETTINGS			it	v	1
IDS_MI_VIDEO_SETTINGS			nl	V	1
IDS_MI_VIDEO_SETTINGS			sv	G	1
IDS_MI_VIDEO_SETTINGS			tr	G	1

IDS_MI_DEVICEMANAGER			en	P	1
IDS_MI_DEVICEMANAGER			da	E	1
IDS_MI_DEVICEMANAGER			de	P	1
IDS_MI_DEVICEMANAGER			hu	P	1
IDS_MI_DEVICEMANAGER			it	p	2
IDS_MI_DEVICEMANAGER			nl	a	2
IDS_MI_DEVICEMANAGER			sv	k	1
IDS_MI_DEVICEMANAGER			tr	v	1

IDS_MI_JOY_SETTINGS			en	J	1
IDS_MI_JOY_SETTINGS			da	J	1
IDS_MI_JOY_SETTINGS			de	J	1
IDS_MI_JOY_SETTINGS			hu	o	1
IDS_MI_JOY_SETTINGS			it	j	1
IDS_MI_JOY_SETTINGS			nl	J	1
IDS_MI_JOY_SETTINGS			sv	s	2
IDS_MI_JOY_SETTINGS			tr	J	1

IDS_MI_USERPORT_JOY_SETTINGS	**	U	1
IDS_MI_USERPORT_JOY_SETTINGS	da	B	1
IDS_MI_USERPORT_JOY_SETTINGS	sv	a	2

IDS_MI_SIDCART_JOY_SETTINGS	**	S	1

IDS_MI_KEYBOARD_SETTINGS		en	K	1
IDS_MI_KEYBOARD_SETTINGS		da	T	1
IDS_MI_KEYBOARD_SETTINGS		de	T	1
IDS_MI_KEYBOARD_SETTINGS		hu	B	1
IDS_MI_KEYBOARD_SETTINGS		it	t	2
IDS_MI_KEYBOARD_SETTINGS		nl	T	1
IDS_MI_KEYBOARD_SETTINGS		sv	T	1
IDS_MI_KEYBOARD_SETTINGS		tr	K	1

IDS_MI_SOUND_SETTINGS			en	o	1
IDS_MI_SOUND_SETTINGS			da	y	1
IDS_MI_SOUND_SETTINGS			de	o	1
IDS_MI_SOUND_SETTINGS			it	u	1
IDS_MI_SOUND_SETTINGS			nl	e	1
IDS_MI_SOUND_SETTINGS			sv	j	1
IDS_MI_SOUND_SETTINGS			tr	S	1

IDS_MI_ROM_SETTINGS			**	R	1

IDS_MI_RAM_SETTINGS			**	M	1
IDS_MI_RAM_SETTINGS			de	A	1

IDS_MI_DATASETTE_SETTINGS		**	a	1
IDS_MI_DATASETTE_SETTINGS		it	e	1

IDS_MI_MOUSE_SETTINGS			**	u	1
IDS_MI_MOUSE_SETTINGS			hu	b	1

IDS_MI_SID_SETTINGS			**	I	1
IDS_MI_SID_SETTINGS			it	I	2

IDS_MI_RS232_SETTINGS			**	2	1

IDS_MI_REU_SETTINGS			**	R	1

IDS_MI_GEORAM_SETTINGS		**	G	1

IDS_MI_RAMCART_SETTINGS		**	R	1

IDS_MI_DQBB_SETTINGS			**	D	1
IDS_MI_DQBB_SETTINGS			sv	d	1

IDS_MI_EXPERT_SETTINGS		**	E	1

IDS_MI_ISEPIC_SETTINGS		**	S	1

IDS_MI_MMC64_SETTINGS			**	M	1

IDS_MI_MMCREPLAY_SETTINGS		**	C	1

IDS_MI_MAGICVOICE_SETTINGS		**	o	1
IDS_MI_MAGICVOICE_SETTINGS		it	o	3

IDS_MI_MIDI_SETTINGS			**	I	1
IDS_MI_MIDI_SETTINGS			it	I	2

IDS_MI_DIGIMAX_SETTINGS		**	D	1

IDS_MI_LIGHTPEN_SETTINGS		en	L	1
IDS_MI_LIGHTPEN_SETTINGS		da	L	1
IDS_MI_LIGHTPEN_SETTINGS		de	L	1
IDS_MI_LIGHTPEN_SETTINGS		hu	F	1
IDS_MI_LIGHTPEN_SETTINGS		it	p	2
IDS_MI_LIGHTPEN_SETTINGS		nl	L	1
IDS_MI_LIGHTPEN_SETTINGS		sv	l	3
IDS_MI_LIGHTPEN_SETTINGS		tr	I	1

IDS_MI_IDE64_SETTINGS			**	I	1
IDS_MI_IDE64_SETTINGS			it	I	2

IDS_MI_TFE_SETTINGS			**	E	1

IDS_MI_ACIA_SETTINGS			**	A	1

IDS_MI_RS232USER_SETTINGS		**	2	1

IDS_MI_SETTINGS_SAVE			en	S	1
IDS_MI_SETTINGS_SAVE			da	s	1
IDS_MI_SETTINGS_SAVE			de	s	2
IDS_MI_SETTINGS_SAVE			fr	E	1
IDS_MI_SETTINGS_SAVE			hu	m	1
IDS_MI_SETTINGS_SAVE			it	S	1
IDS_MI_SETTINGS_SAVE			nl	s	2
IDS_MI_SETTINGS_SAVE			sv	S	1
IDS_MI_SETTINGS_SAVE			tr	k	1

IDS_MI_SETTINGS_LOAD			en	L	1
IDS_MI_SETTINGS_LOAD			da	l	1
IDS_MI_SETTINGS_LOAD			de	L	1
IDS_MI_SETTINGS_LOAD			fr	C	1
IDS_MI_SETTINGS_LOAD			hu	b	2
IDS_MI_SETTINGS_LOAD			it	C	1
IDS_MI_SETTINGS_LOAD			nl	l	1
IDS_MI_SETTINGS_LOAD			sv	L	1
IDS_MI_SETTINGS_LOAD			tr	l	3

IDS_MI_SETTINGS_DEFAULT		en	f	1
IDS_MI_SETTINGS_DEFAULT		da	d	1
IDS_MI_SETTINGS_DEFAULT		de	w	1
IDS_MI_SETTINGS_DEFAULT		fr	f	1
IDS_MI_SETTINGS_DEFAULT		hu	b	1
IDS_MI_SETTINGS_DEFAULT		it	R	1
IDS_MI_SETTINGS_DEFAULT		nl	d	2
IDS_MI_SETTINGS_DEFAULT		sv	Å	1
IDS_MI_SETTINGS_DEFAULT		tr	V	1

IDS_MI_SAVE_SETTINGS_ON_EXIT	en	x	1
IDS_MI_SAVE_SETTINGS_ON_EXIT	da	l	3
IDS_MI_SAVE_SETTINGS_ON_EXIT	fr	r	4
IDS_MI_SAVE_SETTINGS_ON_EXIT	hu	i	1
IDS_MI_SAVE_SETTINGS_ON_EXIT	it	s	2
IDS_MI_SAVE_SETTINGS_ON_EXIT	nl	t	2
IDS_MI_SAVE_SETTINGS_ON_EXIT	sv	a	4
IDS_MI_SAVE_SETTINGS_ON_EXIT	tr	k	1

IDS_MI_CONFIRM_ON_EXIT		en	C	1
IDS_MI_CONFIRM_ON_EXIT		da	B	1
IDS_MI_CONFIRM_ON_EXIT		de	B	1
IDS_MI_CONFIRM_ON_EXIT		fr	C	1
IDS_MI_CONFIRM_ON_EXIT		hu	M	1
IDS_MI_CONFIRM_ON_EXIT		it	C	1
IDS_MI_CONFIRM_ON_EXIT		nl	u	1
IDS_MI_CONFIRM_ON_EXIT		sv	B	1
IDS_MI_CONFIRM_ON_EXIT		tr	t	2

IDS_MI_LANG_EN				en	E	1
IDS_MI_LANG_EN				da	E	1
IDS_MI_LANG_EN				de	E	1
IDS_MI_LANG_EN				fr	A	1
IDS_MI_LANG_EN				hu	A	1
IDS_MI_LANG_EN				it	n	1
IDS_MI_LANG_EN				nl	E	1
IDS_MI_LANG_EN				sv	E	1
IDS_MI_LANG_EN				tr	e	1

IDS_MI_LANG_DA				en	a	1
IDS_MI_LANG_DA				da	a	1
IDS_MI_LANG_DA				de	ä	1
IDS_MI_LANG_DA				hu	D	1
IDS_MI_LANG_DA				it	a	1
IDS_MI_LANG_DA				nl	e	1
IDS_MI_LANG_DA				sv	a	1
IDS_MI_LANG_DA				tr	n	1

IDS_MI_LANG_DE				en	G	1
IDS_MI_LANG_DE				da	T	1
IDS_MI_LANG_DE				de	D	1
IDS_MI_LANG_DE				fr	A	1
IDS_MI_LANG_DE				hu	N	1
IDS_MI_LANG_DE				it	T	1
IDS_MI_LANG_DE				nl	D	1
IDS_MI_LANG_DE				sv	T	1
IDS_MI_LANG_DE				tr	A	1

IDS_MI_LANG_FR				**	F	1

IDS_MI_LANG_HU				en	H	1
IDS_MI_LANG_HU				da	U	1
IDS_MI_LANG_HU				de	U	1
IDS_MI_LANG_HU				hu	M	1
IDS_MI_LANG_HU				it	U	1
IDS_MI_LANG_HU				nl	H	1
IDS_MI_LANG_HU				sv	U	1
IDS_MI_LANG_HU				tr	M	1

IDS_MI_LANG_IT				**	I	1
IDS_MI_LANG_IT				hu	O	1
IDS_MI_LANG_IT				tr	Ý	1

IDS_MI_LANG_KO				en	K	1
IDS_MI_LANG_KO				de	K	1
IDS_MI_LANG_KO				nl	K	1

IDS_MI_LANG_NL				en	D	1
IDS_MI_LANG_NL				da	H	1
IDS_MI_LANG_NL				de	H	1
IDS_MI_LANG_NL				fr	H	1
IDS_MI_LANG_NL				hu	H	1
IDS_MI_LANG_NL				it	O	1
IDS_MI_LANG_NL				nl	N	1
IDS_MI_LANG_NL				sv	N	1
IDS_MI_LANG_NL				tr	d	1

IDS_MI_LANG_PL				**	P	1
IDS_MI_LANG_PL				hu	L	1

IDS_MI_LANG_RU				en	R	1
IDS_MI_LANG_RU				de	R	1
IDS_MI_LANG_RU				nl	R	1

IDS_MI_LANG_SV				**	S	1
IDS_MI_LANG_SV				nl	Z	1
IDS_MI_LANG_SV				tr	s	1

IDS_MI_LANG_TR				**	T	1
IDS_MI_LANG_TR				it	r	1

IDS_MI_CMDLINE				en	o	2
IDS_MI_CMDLINE				da	o	2
IDS_MI_CMDLINE				de	O	1
IDS_MI_CMDLINE				fr	O	1
IDS_MI_CMDLINE				hu	o	2
IDS_MI_CMDLINE				it	O	1
IDS_MI_CMDLINE				nl	o	3
IDS_MI_CMDLINE				sv	f	1
IDS_MI_CMDLINE				tr	o	1

IDS_MI_CONTRIBUTORS			en	C	1
IDS_MI_CONTRIBUTORS			da	B	1
IDS_MI_CONTRIBUTORS			fr	C	1
IDS_MI_CONTRIBUTORS			hu	K	1
IDS_MI_CONTRIBUTORS			it	C	1
IDS_MI_CONTRIBUTORS			nl	M	1
IDS_MI_CONTRIBUTORS			sv	B	1
IDS_MI_CONTRIBUTORS			tr	c	1

IDS_MI_LICENSE				**	L	1

IDS_MI_WARRANTY				en	w	1
IDS_MI_WARRANTY				da	g	2
IDS_MI_WARRANTY				de	G	1
IDS_MI_WARRANTY				fr	g	1
IDS_MI_WARRANTY				hu	g	1
IDS_MI_WARRANTY				it	g	1
IDS_MI_WARRANTY				nl	g	1
IDS_MI_WARRANTY				sv	g	2
IDS_MI_WARRANTY				tr	v	1

IDS_MI_SIDCART_SETTINGS		**	S	1

IDS_MI_MON_OPEN				en	O	1
IDS_MI_MON_OPEN				da	Å	1
IDS_MI_MON_OPEN				de	Ö	1
IDS_MI_MON_OPEN				fr	O	1
IDS_MI_MON_OPEN				hu	M	1
IDS_MI_MON_OPEN				it	A	1
IDS_MI_MON_OPEN				nl	O	1
IDS_MI_MON_OPEN				sv	Ö	1
IDS_MI_MON_OPEN				tr	A	1

IDS_MI_MON_SAVE				en	S	1
IDS_MI_MON_SAVE				da	G	1
IDS_MI_MON_SAVE				de	S	1
IDS_MI_MON_SAVE				fr	E	1
IDS_MI_MON_SAVE				hu	e	1
IDS_MI_MON_SAVE				it	S	1
IDS_MI_MON_SAVE				nl	s	1
IDS_MI_MON_SAVE				sv	S	1
IDS_MI_MON_SAVE				tr	K	1

IDS_MI_MON_PRINT			en	P	1
IDS_MI_MON_PRINT			da	P	1
IDS_MI_MON_PRINT			de	D	1
IDS_MI_MON_PRINT			fr	I	1
IDS_MI_MON_PRINT			hu	N	1
IDS_MI_MON_PRINT			it	p	1
IDS_MI_MON_PRINT			nl	P	1
IDS_MI_MON_PRINT			sv	u	1
IDS_MI_MON_PRINT			tr	Y	1

IDS_MI_MON_EXIT				en	x	1
IDS_MI_MON_EXIT				da	A	1
IDS_MI_MON_EXIT				de	x	1
IDS_MI_MON_EXIT				it	s	1
IDS_MI_MON_EXIT				nl	f	1
IDS_MI_MON_EXIT				sv	A	1
IDS_MI_MON_EXIT				tr	k	1

IDS_MI_MON_STOP_DEBUG			en	S	1
IDS_MI_MON_STOP_DEBUG			da	S	1
IDS_MI_MON_STOP_DEBUG			de	S	1
IDS_MI_MON_STOP_DEBUG			fr	A	1
IDS_MI_MON_STOP_DEBUG			hu	e	1
IDS_MI_MON_STOP_DEBUG			it	I	1
IDS_MI_MON_STOP_DEBUG			nl	S	1
IDS_MI_MON_STOP_DEBUG			sv	A	1
IDS_MI_MON_STOP_DEBUG			tr	D	1

IDS_MI_MON_STOP_EXEC			en	x	1
IDS_MI_MON_STOP_EXEC			da	k	1
IDS_MI_MON_STOP_EXEC			de	A	1
IDS_MI_MON_STOP_EXEC			fr	x	1
IDS_MI_MON_STOP_EXEC			hu	l	1
IDS_MI_MON_STOP_EXEC			it	s	1
IDS_MI_MON_STOP_EXEC			nl	U	1
IDS_MI_MON_STOP_EXEC			sv	x	1
IDS_MI_MON_STOP_EXEC			tr	r	1

IDS_MI_MON_STEP_INTO			**	i	1
IDS_MI_MON_STEP_INTO			hu	e	1
IDS_MI_MON_STEP_INTO			it	i	2
IDS_MI_MON_STEP_INTO			tr	A	1

IDS_MI_MON_STEP_OVER			en	o	1
IDS_MI_MON_STEP_OVER			da	o	1
IDS_MI_MON_STEP_OVER			de	ü	1
IDS_MI_MON_STEP_OVER			hu	t	1
IDS_MI_MON_STEP_OVER			it	f	1
IDS_MI_MON_STEP_OVER			nl	o	1
IDS_MI_MON_STEP_OVER			sv	ö	1
IDS_MI_MON_STEP_OVER			tr	g	1

IDS_MI_MON_SKIP_RETURN		**	r	1
IDS_MI_MON_SKIP_RETURN		fr	r	2
IDS_MI_MON_SKIP_RETURN		hu	v	1
IDS_MI_MON_SKIP_RETURN		nl	t	3

IDS_MI_MON_GOTO_CURSOR		**	c	1
IDS_MI_MON_GOTO_CURSOR		hu	k	1
IDS_MI_MON_GOTO_CURSOR		sv	m	1

IDS_MI_MON_EVAL				en	E	1
IDS_MI_MON_EVAL				da	E	1
IDS_MI_MON_EVAL				de	u	1
IDS_MI_MON_EVAL				fr	u	1
IDS_MI_MON_EVAL				hu	K	1
IDS_MI_MON_EVAL				it	V	1
IDS_MI_MON_EVAL				nl	E	1
IDS_MI_MON_EVAL				sv	U	1
IDS_MI_MON_EVAL				tr	e	1

IDS_MI_MON_CURRENT			en	C	1
IDS_MI_MON_CURRENT			da	A	1
IDS_MI_MON_CURRENT			de	n	1
IDS_MI_MON_CURRENT			hu	J	1
IDS_MI_MON_CURRENT			it	c	1
IDS_MI_MON_CURRENT			nl	H	1
IDS_MI_MON_CURRENT			sv	A	1
IDS_MI_MON_CURRENT			tr	G	1

IDS_MI_MON_WND_EVAL			en	w	1
IDS_MI_MON_WND_EVAL			da	v	2
IDS_MI_MON_WND_EVAL			de	f	1
IDS_MI_MON_WND_EVAL			fr	v	1
IDS_MI_MON_WND_EVAL			hu	K	1
IDS_MI_MON_WND_EVAL			it	F	1
IDS_MI_MON_WND_EVAL			nl	a	1
IDS_MI_MON_WND_EVAL			sv	f	1
IDS_MI_MON_WND_EVAL			tr	p	2

IDS_MI_MON_WND_REG			**	R	1
IDS_MI_MON_WND_REG			it	r	1
IDS_MI_MON_WND_REG			tr	r	1

IDS_MI_MON_WND_MEM			en	M	1
IDS_MI_MON_WND_MEM			da	H	1
IDS_MI_MON_WND_MEM			de	p	1
IDS_MI_MON_WND_MEM			fr	m	1
IDS_MI_MON_WND_MEM			hu	M	1
IDS_MI_MON_WND_MEM			it	m	1
IDS_MI_MON_WND_MEM			nl	G	1
IDS_MI_MON_WND_MEM			sv	M	1
IDS_MI_MON_WND_MEM			tr	B	1

IDS_MI_MON_WND_DIS			**	D	1
IDS_MI_MON_WND_DIS			hu	V	1
IDS_MI_MON_WND_DIS			it	d	2

IDS_MI_MON_WND_CONSOLE		en	C	1
IDS_MI_MON_WND_CONSOLE		da	K	1
IDS_MI_MON_WND_CONSOLE		de	K	1
IDS_MI_MON_WND_CONSOLE		fr	C	1
IDS_MI_MON_WND_CONSOLE		hu	K	1
IDS_MI_MON_WND_CONSOLE		it	c	1
IDS_MI_MON_WND_CONSOLE		nl	C	1
IDS_MI_MON_WND_CONSOLE		sv	K	1
IDS_MI_MON_WND_CONSOLE		tr	c	1

IDS_MI_MON_COMPUTER			en	C	1
IDS_MI_MON_COMPUTER			da	C	1
IDS_MI_MON_COMPUTER			fr	O	1
IDS_MI_MON_COMPUTER			hu	S	1
IDS_MI_MON_COMPUTER			it	C	1
IDS_MI_MON_COMPUTER			nl	C	1
IDS_MI_MON_COMPUTER			sv	D	1
IDS_MI_MON_COMPUTER			tr	B	1

IDS_MI_MON_DRIVE8			**	8	1

IDS_MI_MON_DRIVE9			**	9	1

IDS_MI_MON_CASCADE			en	C	1
IDS_MI_MON_CASCADE			da	K	1
IDS_MI_MON_CASCADE			de	K	1
IDS_MI_MON_CASCADE			fr	C	1
IDS_MI_MON_CASCADE			hu	K	1
IDS_MI_MON_CASCADE			it	c	1
IDS_MI_MON_CASCADE			nl	A	1
IDS_MI_MON_CASCADE			sv	Ö	1
IDS_MI_MON_CASCADE			tr	B	1

IDS_MI_MON_TILE_VERT			en	v	1
IDS_MI_MON_TILE_VERT			da	S	1
IDS_MI_MON_TILE_VERT			de	V	1
IDS_MI_MON_TILE_VERT			fr	v	1
IDS_MI_MON_TILE_VERT			hu	v	1
IDS_MI_MON_TILE_VERT			it	v	1
IDS_MI_MON_TILE_VERT			nl	N	1
IDS_MI_MON_TILE_VERT			sv	S	1
IDS_MI_MON_TILE_VERT			tr	D	1

IDS_MI_MON_TILE_HORIZ			en	h	1
IDS_MI_MON_TILE_HORIZ			da	O	1
IDS_MI_MON_TILE_HORIZ			de	H	1
IDS_MI_MON_TILE_HORIZ			fr	h	1
IDS_MI_MON_TILE_HORIZ			hu	f	1
IDS_MI_MON_TILE_HORIZ			it	o	1
IDS_MI_MON_TILE_HORIZ			nl	e	2
IDS_MI_MON_TILE_HORIZ			sv	Ö	1
IDS_MI_MON_TILE_HORIZ			tr	Y	1

IDS_MI_MON_ARRANGE_ICONS		en	A	1
IDS_MI_MON_ARRANGE_ICONS		da	A	1
IDS_MI_MON_ARRANGE_ICONS		de	A	1
IDS_MI_MON_ARRANGE_ICONS		fr	A	1
IDS_MI_MON_ARRANGE_ICONS		hu	I	1
IDS_MI_MON_ARRANGE_ICONS		it	D	1
IDS_MI_MON_ARRANGE_ICONS		nl	R	1
IDS_MI_MON_ARRANGE_ICONS		sv	A	1
IDS_MI_MON_ARRANGE_ICONS		tr	S	1


# resacia.rc

IDS_ACIA_ENABLE		en	E	1
IDS_ACIA_ENABLE		da	A	1
IDS_ACIA_ENABLE		de	e	2
IDS_ACIA_ENABLE		fr	A	1
IDS_ACIA_ENABLE		hu	e	1
IDS_ACIA_ENABLE		it	A	1
IDS_ACIA_ENABLE		nl	A	1
IDS_ACIA_ENABLE		sv	A	1
IDS_ACIA_ENABLE		tr	e	1


# resc64.rc

IDS_MI_PLUS60K_SETTINGS	**	6	1

IDS_MI_PLUS256K_SETTINGS	**	5	1

IDS_MI_C64_256K_SETTINGS	**	2	1


# resc64_256k.rc

IDS_C64_256K_ENABLE	en	E	1
IDS_C64_256K_ENABLE	da	A	1
IDS_C64_256K_ENABLE	de	a	1
IDS_C64_256K_ENABLE	fr	A	1
IDS_C64_256K_ENABLE	hu	e	1
IDS_C64_256K_ENABLE	it	A	1
IDS_C64_256K_ENABLE	nl	A	1
IDS_C64_256K_ENABLE	sv	A	1
IDS_C64_256K_ENABLE	sv	e	1


# resdigimax.rc

IDS_DIGIMAX_ENABLE	en	E	1
IDS_DIGIMAX_ENABLE	da	A	1
IDS_DIGIMAX_ENABLE	de	e	1
IDS_DIGIMAX_ENABLE	it	A	1
IDS_DIGIMAX_ENABLE	nl	A	1
IDS_DIGIMAX_ENABLE	sv	A	1
IDS_DIGIMAX_ENABLE	tr	e	1


# resdqbb.rc

IDS_DQBB_ENABLE			en	E	1
IDS_DQBB_ENABLE			da	A	1
IDS_DQBB_ENABLE			de	e	2
IDS_DQBB_ENABLE			hu	e	1
IDS_DQBB_ENABLE			it	A	1
IDS_DQBB_ENABLE			nl	A	1
IDS_DQBB_ENABLE			sv	A	1
IDS_DQBB_ENABLE			tr	e	1

IDS_DQBB_WRITE_ENABLE		en	S	1
IDS_DQBB_WRITE_ENABLE		da	G	1
IDS_DQBB_WRITE_ENABLE		de	s	1
IDS_DQBB_WRITE_ENABLE		it	S	1
IDS_DQBB_WRITE_ENABLE		nl	s	2
IDS_DQBB_WRITE_ENABLE		sv	S	1
IDS_DQBB_WRITE_ENABLE		tr	s	1


# reseasyflash.rc

IDS_EASYFLASH_JUMPER		en	J	1
IDS_EASYFLASH_JUMPER		da	J	1
IDS_EASYFLASH_JUMPER		de	J	1
IDS_EASYFLASH_JUMPER		hu	j	1
IDS_EASYFLASH_JUMPER		it	P	1
IDS_EASYFLASH_JUMPER		nl	J	1
IDS_EASYFLASH_JUMPER		sv	b	1

IDS_EASYFLASH_AUTOSAVE	en	S	1
IDS_EASYFLASH_AUTOSAVE	da	G	1
IDS_EASYFLASH_AUTOSAVE	de	s	1
IDS_EASYFLASH_AUTOSAVE	hu	l	1
IDS_EASYFLASH_AUTOSAVE	it	S	1
IDS_EASYFLASH_AUTOSAVE	nl	s	1
IDS_EASYFLASH_AUTOSAVE	sv	S	1
IDS_EASYFLASH_AUTOSAVE	tr	s	1

IDS_EASYFLASH_SAVE_NOW	en	n	1
IDS_EASYFLASH_SAVE_NOW	da	n	1
IDS_EASYFLASH_SAVE_NOW	de	n	1
IDS_EASYFLASH_SAVE_NOW	hu	m	2
IDS_EASYFLASH_SAVE_NOW	it	o	1
IDS_EASYFLASH_SAVE_NOW	nl	n	1
IDS_EASYFLASH_SAVE_NOW	sv	n	1
IDS_EASYFLASH_SAVE_NOW	tr	n	1


# resexpert.rc

IDS_EXPERT_ENABLE		en	E	1
IDS_EXPERT_ENABLE		da	E	1
IDS_EXPERT_ENABLE		de	E	1
IDS_EXPERT_ENABLE		it	A	1
IDS_EXPERT_ENABLE		nl	A	1
IDS_EXPERT_ENABLE		sv	A	1
IDS_EXPERT_ENABLE		tr	E	1

IDS_EXPERT_WRITE_ENABLE	en	S	1
IDS_EXPERT_WRITE_ENABLE	da	G	1
IDS_EXPERT_WRITE_ENABLE	de	s	1
IDS_EXPERT_WRITE_ENABLE	it	S	1
IDS_EXPERT_WRITE_ENABLE	nl	s	2
IDS_EXPERT_WRITE_ENABLE	sv	S	1
IDS_EXPERT_WRITE_ENABLE	tr	s	1


# resgeoram.rc

IDS_GEORAM_ENABLE		en	E	1
IDS_GEORAM_ENABLE		da	A	1
IDS_GEORAM_ENABLE		de	e	1
IDS_GEORAM_ENABLE		it	A	1
IDS_GEORAM_ENABLE		nl	A	1
IDS_GEORAM_ENABLE		sv	A	1
IDS_GEORAM_ENABLE		tr	e	1

IDS_GEORAM_WRITE_ENABLE	en	S	1
IDS_GEORAM_WRITE_ENABLE	da	G	1
IDS_GEORAM_WRITE_ENABLE	de	s	1
IDS_GEORAM_WRITE_ENABLE	it	S	1
IDS_GEORAM_WRITE_ENABLE	nl	s	2
IDS_GEORAM_WRITE_ENABLE	sv	S	1
IDS_GEORAM_WRITE_ENABLE	tr	s	1


# reside64.rc

IDS_IDE64_IMAGE_1		**	1	1

IDS_IDE64_IMAGE_2		**	2	1

IDS_IDE64_IMAGE_3		**	3	1

IDS_IDE64_IMAGE_4		**	4	1

IDS_IDE64_GEOMETRY		**	G	1

IDS_IDE64_AUTODETECT		**	A	1
IDS_IDE64_AUTODETECT		it	R	1
IDS_IDE64_AUTODETECT		tr	a	1


# resisepic.rc

IDS_ISEPIC_ENABLE		en	E	1
IDS_ISEPIC_ENABLE		da	A	1
IDS_ISEPIC_ENABLE		de	A	1
IDS_ISEPIC_ENABLE		it	A	1
IDS_ISEPIC_ENABLE		nl	A	1
IDS_ISEPIC_ENABLE		sv	A	1
IDS_ISEPIC_ENABLE		tr	e	1

IDS_ISEPIC_SWITCH		**	I	1

IDS_ISEPIC_WRITE_ENABLE	en	S	1
IDS_ISEPIC_WRITE_ENABLE	da	G	1
IDS_ISEPIC_WRITE_ENABLE	de	s	1
IDS_ISEPIC_WRITE_ENABLE	it	S	1
IDS_ISEPIC_WRITE_ENABLE	nl	s	2
IDS_ISEPIC_WRITE_ENABLE	sv	S	1
IDS_ISEPIC_WRITE_ENABLE	tr	S	1


# reslightpen.rc

IDS_LIGHTPEN_ENABLE	en	E	1
IDS_LIGHTPEN_ENABLE	da	e	1
IDS_LIGHTPEN_ENABLE	de	E	1
IDS_LIGHTPEN_ENABLE	hu	F	1
IDS_LIGHTPEN_ENABLE	it	A	1
IDS_LIGHTPEN_ENABLE	nl	A	1
IDS_LIGHTPEN_ENABLE	sv	l	1


# resmagicvoice.rc

IDS_MAGICVOICE_ENABLE		en	E	1
IDS_MAGICVOICE_ENABLE		de	M	1
IDS_MAGICVOICE_ENABLE		it	A	1
IDS_MAGICVOICE_ENABLE		nl	A	1
IDS_MAGICVOICE_ENABLE		sv	A	1
IDS_MAGICVOICE_ENABLE		tr	e	1


# resmidi.rc

IDS_MIDI_ENABLE		en	E	1
IDS_MIDI_ENABLE		da	A	1
IDS_MIDI_ENABLE		de	e	2
IDS_MIDI_ENABLE		it	A	1
IDS_MIDI_ENABLE		nl	A	1
IDS_MIDI_ENABLE		sv	A	1
IDS_MIDI_ENABLE		tr	e	1


# resmmc64.rc

IDS_MMC64_ENABLE			en	E	1
IDS_MMC64_ENABLE			da	A	1
IDS_MMC64_ENABLE			de	e	2
IDS_MMC64_ENABLE			hu	e	1
IDS_MMC64_ENABLE			it	A	1
IDS_MMC64_ENABLE			nl	A	1
IDS_MMC64_ENABLE			sv	A	1
IDS_MMC64_ENABLE			tr	e	1

IDS_MMC64_FLASHJUMPER			**	F	1
IDS_MMC64_FLASHJUMPER			da	f	1
IDS_MMC64_FLASHJUMPER			sv	f	1

IDS_MMC64_BIOS_SAVE			en	S	1
IDS_MMC64_BIOS_SAVE			da	G	1
IDS_MMC64_BIOS_SAVE			de	s	1
IDS_MMC64_BIOS_SAVE			fr	E	1
IDS_MMC64_BIOS_SAVE			hu	m	1
IDS_MMC64_BIOS_SAVE			it	S	1
IDS_MMC64_BIOS_SAVE			nl	s	1
IDS_MMC64_BIOS_SAVE			sv	S	1
IDS_MMC64_BIOS_SAVE			tr	S	1

IDS_MMC64_BIOS_FILE_LABEL		**	B	1

IDS_MMC64_IMAGE_FILE_LABEL		en	I	1
IDS_MMC64_IMAGE_FILE_LABEL		da	i	1
IDS_MMC64_IMAGE_FILE_LABEL		de	I	1
IDS_MMC64_IMAGE_FILE_LABEL		hu	k	1
IDS_MMC64_IMAGE_FILE_LABEL		it	i	1
IDS_MMC64_IMAGE_FILE_LABEL		nl	e	1
IDS_MMC64_IMAGE_FILE_LABEL		sv	a	1
IDS_MMC64_IMAGE_FILE_LABEL		tr	I	1


# resplus60k.rc

IDS_PLUS60K_ENABLE	en	E	1
IDS_PLUS60K_ENABLE	da	A	1
IDS_PLUS60K_ENABLE	de	e	2
IDS_PLUS60K_ENABLE	fr	A	1
IDS_PLUS60K_ENABLE	hu	e	1
IDS_PLUS60K_ENABLE	it	A	1
IDS_PLUS60K_ENABLE	nl	A	1
IDS_PLUS60K_ENABLE	sv	A	1
IDS_PLUS60K_ENABLE	tr	e	1


# resplus256k.rc

IDS_PLUS256K_ENABLE	en	E	1
IDS_PLUS256K_ENABLE	da	A	1
IDS_PLUS256K_ENABLE	de	e	2
IDS_PLUS256K_ENABLE	fr	A	1
IDS_PLUS256K_ENABLE	hu	e	1
IDS_PLUS256K_ENABLE	it	A	1
IDS_PLUS256K_ENABLE	nl	A	1
IDS_PLUS256K_ENABLE	sv	A	1
IDS_PLUS256K_ENABLE	tr	e	1


# resramcart.rc

IDS_RAMCART_ENABLE		en	E	1
IDS_RAMCART_ENABLE		da	A	1
IDS_RAMCART_ENABLE		de	e	1
IDS_RAMCART_ENABLE		it	A	1
IDS_RAMCART_ENABLE		nl	A	1
IDS_RAMCART_ENABLE		sv	A	1
IDS_RAMCART_ENABLE		tr	e	1

IDS_RAMCART_READONLY		en	R	1
IDS_RAMCART_READONLY		da	K	1
IDS_RAMCART_READONLY		de	r	1
IDS_RAMCART_READONLY		fr	L	1
IDS_RAMCART_READONLY		hu	C	1
IDS_RAMCART_READONLY		it	A	1
IDS_RAMCART_READONLY		nl	l	3
IDS_RAMCART_READONLY		sv	E	1
IDS_RAMCART_READONLY		tr	r	1

IDS_RAMCART_WRITE_ENABLE	en	S	1
IDS_RAMCART_WRITE_ENABLE	da	G	1
IDS_RAMCART_WRITE_ENABLE	de	s	1
IDS_RAMCART_WRITE_ENABLE	it	S	1
IDS_RAMCART_WRITE_ENABLE	nl	s	2
IDS_RAMCART_WRITE_ENABLE	sv	S	1
IDS_RAMCART_WRITE_ENABLE	tr	s	1


# resreu.rc

IDS_REU_ENABLE		en	E	1
IDS_REU_ENABLE		da	A	1
IDS_REU_ENABLE		de	e	1
IDS_REU_ENABLE		fr	A	1
IDS_REU_ENABLE		hu	e	1
IDS_REU_ENABLE		it	A	1
IDS_REU_ENABLE		nl	A	1
IDS_REU_ENABLE		sv	A	1
IDS_REU_ENABLE		tr	e	1

IDS_REU_WRITE_ENABLE	en	S	1
IDS_REU_WRITE_ENABLE	da	G	1
IDS_REU_WRITE_ENABLE	de	s	1
IDS_REU_WRITE_ENABLE	it	S	1
IDS_REU_WRITE_ENABLE	nl	s	2
IDS_REU_WRITE_ENABLE	sv	S	1
IDS_REU_WRITE_ENABLE	tr	s	1


# resrs232user.rc

IDS_RS232USER_ENABLE		en	E	1
IDS_RS232USER_ENABLE		da	A	1
IDS_RS232USER_ENABLE		de	e	2
IDS_RS232USER_ENABLE		fr	A	1
IDS_RS232USER_ENABLE		hu	e	2
IDS_RS232USER_ENABLE		it	A	1
IDS_RS232USER_ENABLE		nl	A	1
IDS_RS232USER_ENABLE		sv	A	1
IDS_RS232USER_ENABLE		tr	e	2


# ressoundexpander.rc

IDS_SFX_SOUNDEXPANDER_ENABLE	en	E	1
IDS_SFX_SOUNDEXPANDER_ENABLE	da	A	1
IDS_SFX_SOUNDEXPANDER_ENABLE	de	e	3
IDS_SFX_SOUNDEXPANDER_ENABLE	hu	e	2
IDS_SFX_SOUNDEXPANDER_ENABLE	it	A	1
IDS_SFX_SOUNDEXPANDER_ENABLE	nl	A	1
IDS_SFX_SOUNDEXPANDER_ENABLE	sv	A	1


# restfe.rc

IDS_TFE_ETHERNET	**	E	1

IDS_TFE_INTERFACE	**	I	1
IDS_TFE_INTERFACE	de	i	1
IDS_TFE_INTERFACE	sv	G	1
IDS_TFE_INTERFACE	tr	i	1


# resvicii.rc

IDS_VICII_NORMALBORDERS		**	N	1

IDS_VICII_FULLBORDERS			en	F	1
IDS_VICII_FULLBORDERS			da	F	1
IDS_VICII_FULLBORDERS			de	V	1
IDS_VICII_FULLBORDERS			hu	T	1
IDS_VICII_FULLBORDERS			it	I	1
IDS_VICII_FULLBORDERS			nl	V	1
IDS_VICII_FULLBORDERS			sv	F	1
IDS_VICII_FULLBORDERS			tr	T	1

IDS_VICII_DEBUGBORDERS		en	D	1
IDS_VICII_DEBUGBORDERS		da	D	1
IDS_VICII_DEBUGBORDERS		de	D	1
IDS_VICII_DEBUGBORDERS		hu	N	1
IDS_VICII_DEBUGBORDERS		it	D	1
IDS_VICII_DEBUGBORDERS		nl	D	1
IDS_VICII_DEBUGBORDERS		sv	F	1
IDS_VICII_DEBUGBORDERS		tr	H	1

IDS_VICII_SPRITECOLL			en	s	1
IDS_VICII_SPRITECOLL			da	s	1
IDS_VICII_SPRITECOLL			de	s	1
IDS_VICII_SPRITECOLL			hu	S	1
IDS_VICII_SPRITECOLL			it	s	3
IDS_VICII_SPRITECOLL			nl	s	1
IDS_VICII_SPRITECOLL			sv	s	1
IDS_VICII_SPRITECOLL			tr	y	1

IDS_VICII_BACKCOLL			en	c	1
IDS_VICII_BACKCOLL			da	b	1
IDS_VICII_BACKCOLL			de	K	1
IDS_VICII_BACKCOLL			hu	h	1
IDS_VICII_BACKCOLL			it	C	1
IDS_VICII_BACKCOLL			nl	b	1
IDS_VICII_BACKCOLL			sv	b	1
IDS_VICII_BACKCOLL			tr	r	3

IDS_VICII_LUMINANCE			en	L	1
IDS_VICII_LUMINANCE			da	l	1
IDS_VICII_LUMINANCE			de	l	1
IDS_VICII_LUMINANCE			fr	l	3
IDS_VICII_LUMINANCE			hu	f	1
IDS_VICII_LUMINANCE			it	L	1
IDS_VICII_LUMINANCE			nl	l	1
IDS_VICII_LUMINANCE			sv	l	1
IDS_VICII_LUMINANCE			tr	l	1
