Numeric 005 Documentation
(c) 2002-2005 codemastr (Dominick Meglio) [codemastr@unrealircd.com]
(c) 2005-2009 syzop (Bram Matthys) [syzop@vulnscan.org]

Numeric 005 allows the server to inform the client of any protocol specific features in the
IRCd.  The numeric is sent at connection time immediately after numeric 004. Additionally
the numeric is sent when a /version request is made by a local user, for remote users
numeric 105 is used but contains the same information.

Due to the limit imposed by RFC1459 on both the buffer size (512) and the amount of
parameters that can be sent in a single command (15) a total of 13 parameters may be
specified in each 005. Because of this, a client must be able to accept multiple 005s
consecutively. The format for the 005 message is as follows:

":" <servername> "005" SPACE <nickname> SPACE <token[=value]> SPACE ... ":are supported
by this server"

Currently UnrealIRCd supports several tokens that are included in numeric 005. A list of
all tokens, their respective value and a brief description are listed below.

Unreal attempts to follow the proposed ISupport standard as much as possible. Unreal only
ignores the standard in one regard, the TARGMAX token. This token is believed to be 
impractical and technically impossible to correctly implement due to existing limitations
in the standard. Therefore, this token is not currently supported. 

Unreal does additionally provide a few tokens which are not specified in the standard, these
include: HCN, AWAYLEN, WATCH, SILENCE, EXTBAN, ELIST, CMDS, NAMESX, UHNAMES, and WATCHOPTS.
Unreal also maintains a few legacy tokens such as MAXCHANNELS and WALLCHOPS to ensure
compatibility until the ISupport standard is more widely accepted by clients.

Token         Value           Default Value                Description
------------------------------------------------------------------------------------------------
MAP           none            none                         Informs the client that the /map 
                                                           command is present. [Obsolete]

KNOCK         none            none                         Informs the client that the /knock
                                                           command is present. [Obsolete]

SAFELIST      none            none                         The LIST command is sent in 
                                                           multiple iterations so that the
                                                           client's queue does not get filled
                                                           causing the user to be killed.

HCN           none            none                         The server supports the HCN
                                                           (Hybrid Connect Notice) protocol.

MAXCHANNELS   number          10                           The maximum number of channels a
                                                           user may join. [Deprecated]

MAXBANS       number          60                           The maximum number of bans that
                                                           may be placed for a channel.
                                                           [Obsolete]

NICKLEN       number          30                           Maximum length of a user's
                                                           nickname.

TOPICLEN      number          307                          Maximum length of a channel's
                                                           topic.

KICKLEN       number          307                          Maximum length of a kick reason.

MAXTARGETS    number          20                           Maximum targets for the PRIVMSG
                                                           command.

AWAYLEN       number          307                          Maximum length of an away message.

WALLCHOPS     none            none                         Indicates that you may use
                                                           NOTICE/PRIVMSG to send to +ohv by
                                                           using PRIVMSG/NOTICE [@|%|+]#channel.
                                                           [Deprecated]
 
WATCH         number          128                          Indicates the presence of the
                                                           WATCH command and specifies the
                                                           maximum number of watch entries.

SILENCE       number          15                           Indicates the maximum number of
                                                           entries on the silence list.

MODES         number          13                           Indicates the number of channel
                                                           modes with parameters that may be
                                                           sent at one time.

CHANTYPES     chars           #                            Indicates the prefixes available
                                                           for channels.
 
PREFIX        (modes)prefixes (qaohv)~&@%+                 Indicates the modes on a channel
                                                           that corespond to the given
                                                           nickname prefixes.

CHANMODES     A,B,C,D         be,kfL,lj,                   Specifies how each channel mode is
                              psmntirRcOAQKVHGCuzNSMT      set/unset. The A section specifies
                                                           modes that add a nick/mask to a
                                                           list. The B section specifies
                                                           modes that require a parameter
                                                           to be both set and unset. The C
                                                           section specifies modes that
                                                           only require a parameter to be
                                                           set, and the D section
                                                           specifies modes that require no
                                                           parameters.

NETWORK       string          no default value             Specifies the name of the
                                                           network that the server is
                                                           connected to.

CASEMAPPING   string          ascii                        Specifies what definition the
                                                           server uses when determining if
                                                           characters are upper/lowercase
                                                           of eachother.

EXTBAN        prefix,types    ~,cqnr                       Specifies what extbans are
                                                           supported by the server. The prefix
                                                           defines which character indicates
                                                           an extban and the types defines
                                                           which extbans the server supports.

ELIST         flags           MNUCT                        Specifies the set of extended LIST
                                                           options supported. The M flag 
                                                           indicates mask based searching,
                                                           the N flag indicates negative
                                                           mask based searching. The U flag
                                                           means support for user count
                                                           searching. The C flag allows channel
                                                           creation time searching, and the T
                                                           flag allows topic set time 
                                                           searching.

CMDS          commands        MAP,KNOCK,DCCALLOW,USERIP    Specifies a series of commands that
                                                           can be useful for the client to know
                                                           exist as they may provide a more
                                                           efficient means for the client to
                                                           accomplish a specific task. This
                                                           token replaces the MAP and KNOCK
                                                           tokens.

STATUSMSG     flags           ~&@%+                        Specifies the mode flags that may
                                                           prefix a channel name in a PRIVMSG
                                                           or NOTICE to limit who receives the
                                                           message to only those with a certain
                                                           level of access. This token will
                                                           replace the WALLCHOPS token.

EXCEPTS       none            none                         Indicates that channel ban exceptions
                                                           (+e) are supported by the server.

INVEX         none            none                         Indicates that channel invite
                                                           exceptions (+I) are supported by
                                                           the server.

MAXLIST       mode:num,...    b:60,e:60,I:60               Specifies the maximum number of 
                                                           entries that may be added to a 
                                                           particular mode list (type A modes).
                                                           This token replaces MAXBANS.

CHANLIMIT     pfx:num,...     #:10                         Specifies the maximum number of 
                                                           channels with the specified prefix
                                                           that a user may join at one time.
                                                           This token will replace MAXCHANNELS.

CHANNELLEN    number          32                           Provides the maximum length of a
                                                           channel name that a user can create.

NAMESX        none            none                         Indicates that extended /NAMES info
                                                           is available on this server. If the
                                                           client sends "PROTOCTL NAMESX" then
                                                           the server will, from then on, send
                                                           all channel rights in a NAMES reply
                                                           instead of only the highest right
                                                           (eg: @+Person instead of @Person).

UHNAMES       none            none                         Indicates that (other) extended
                                                           /NAMES info is available on the
                                                           server. If the client sends
                                                           "PROTOCTL UHNAMES" then the server
                                                           will, from then on, send user@host
                                                           information in a NAMES reply
                                                           (eg: @nick!ident@hostname).

WATCHOPTS     flags           A                            WATCH options supported. 'A' means
                                                           Away Notification is available.
