(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1)
    (drawings 18)
    (tracks 1081)
    (zones 0)
    (modules 16)
    (nets 64)
  )
  (page User 135.458 101.6)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 67.818 24.384)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(J1-Pad2)")
  (net 4 /~WR)
  (net 5 /~RD)
  (net 6 /~CS_ROM)
  (net 7 /AD0)
  (net 8 /AD1)
  (net 9 /AD2)
  (net 10 /AD3)
  (net 11 /AD4)
  (net 12 /AD5)
  (net 13 /AD6)
  (net 14 /AD7)
  (net 15 /AD8)
  (net 16 /AD9)
  (net 17 /AD10)
  (net 18 /AD11)
  (net 19 /AD12)
  (net 20 /AD13)
  (net 21 /AD14)
  (net 22 /AD15)
  (net 23 /A16)
  (net 24 /A17)
  (net 25 /A18)
  (net 26 /A19)
  (net 27 /A20)
  (net 28 /A21)
  (net 29 /A22)
  (net 30 /A23)
  (net 31 "Net-(J1-Pad30)")
  (net 32 "Net-(U1-Pad12)")
  (net 33 "Net-(U3-Pad13)")
  (net 34 /A3)
  (net 35 /A2)
  (net 36 /A0)
  (net 37 /A1)
  (net 38 "Net-(U4-Pad13)")
  (net 39 /A7)
  (net 40 /A6)
  (net 41 /A4)
  (net 42 /A5)
  (net 43 "Net-(U5-Pad13)")
  (net 44 /A11)
  (net 45 /A10)
  (net 46 /A8)
  (net 47 /A9)
  (net 48 "Net-(U6-Pad13)")
  (net 49 "Net-(U6-Pad12)")
  (net 50 /A15)
  (net 51 /A14)
  (net 52 /A12)
  (net 53 /A13)
  (net 54 "Net-(U7-Pad17)")
  (net 55 "Net-(U7-Pad16)")
  (net 56 /~LD)
  (net 57 /CLK)
  (net 58 /U6-~EN)
  (net 59 /U5-~EN)
  (net 60 /U4-~EN)
  (net 61 /U5-MAX)
  (net 62 /U4-MAX)
  (net 63 /U3-MAX)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A22)
    (add_net /A23)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AD0)
    (add_net /AD1)
    (add_net /AD10)
    (add_net /AD11)
    (add_net /AD12)
    (add_net /AD13)
    (add_net /AD14)
    (add_net /AD15)
    (add_net /AD2)
    (add_net /AD3)
    (add_net /AD4)
    (add_net /AD5)
    (add_net /AD6)
    (add_net /AD7)
    (add_net /AD8)
    (add_net /AD9)
    (add_net /CLK)
    (add_net /U3-MAX)
    (add_net /U4-MAX)
    (add_net /U4-~EN)
    (add_net /U5-MAX)
    (add_net /U5-~EN)
    (add_net /U6-~EN)
    (add_net /~CS_ROM)
    (add_net /~LD)
    (add_net /~RD)
    (add_net /~WR)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U6-Pad12)")
    (add_net "Net-(U6-Pad13)")
    (add_net "Net-(U7-Pad16)")
    (add_net "Net-(U7-Pad17)")
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module fles:fles (layer B.Cu) (tedit 0)
    (at 90.418 46.584 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 66.548 32.004 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U6 (at 0 -0.005 90) (layer F.SilkS))
    (fp_text value 74AC191 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /AD12))
    (pad 14 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /CLK))
    (pad 13 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U6-Pad13)"))
    (pad 12 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U6-Pad12)"))
    (pad 11 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~LD))
    (pad 10 smd roundrect (at 2.475 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /AD14))
    (pad 9 smd roundrect (at 2.475 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /AD15))
    (pad 8 smd roundrect (at -2.475 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /A15))
    (pad 6 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /A14))
    (pad 5 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /U6-~EN))
    (pad 3 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /A12))
    (pad 2 smd roundrect (at -2.475 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /A13))
    (pad 1 smd roundrect (at -2.475 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /AD13))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fles:GameBoy_Cartridge_1x32_P1.50mm_Edge (layer F.Cu) (tedit 610CB1B6)
    (at 67.818 24.384 180)
    (descr "Game Boy cartridge edge connector")
    (tags "gameboy cartridge")
    (attr virtual)
    (fp_text reference J1 (at 0 -3.175) (layer F.SilkS))
    (fp_text value GameBoyAdvance_Cartedge (at 0 -8) (layer F.Fab))
    (fp_text user 1 (at -23.876 -3.302) (layer F.SilkS))
    (fp_text user 32 (at 23.368 -3.429) (layer F.SilkS))
    (fp_text user %R (at 0 3) (layer F.Fab))
    (pad 31 connect rect (at 21.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 30 connect rect (at 20.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 31 "Net-(J1-Pad30)"))
    (pad 29 connect rect (at 18.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 30 /A23))
    (pad 28 connect rect (at 17.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 29 /A22))
    (pad 27 connect rect (at 15.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 28 /A21))
    (pad 26 connect rect (at 14.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 27 /A20))
    (pad 25 connect rect (at 12.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 26 /A19))
    (pad 24 connect rect (at 11.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 25 /A18))
    (pad 23 connect rect (at 9.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 24 /A17))
    (pad 22 connect rect (at 8.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 23 /A16))
    (pad 21 connect rect (at 6.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 22 /AD15))
    (pad 20 connect rect (at 5.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 21 /AD14))
    (pad 19 connect rect (at 3.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 20 /AD13))
    (pad 18 connect rect (at 2.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 19 /AD12))
    (pad 17 connect rect (at 0.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 18 /AD11))
    (pad 16 connect rect (at -0.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 17 /AD10))
    (pad 15 connect rect (at -2.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 16 /AD9))
    (pad 14 connect rect (at -3.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 15 /AD8))
    (pad 13 connect rect (at -5.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 14 /AD7))
    (pad 12 connect rect (at -6.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 13 /AD6))
    (pad 11 connect rect (at -8.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 12 /AD5))
    (pad 10 connect rect (at -9.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 11 /AD4))
    (pad 9 connect rect (at -11.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 10 /AD3))
    (pad 8 connect rect (at -12.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 9 /AD2))
    (pad 7 connect rect (at -14.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 8 /AD1))
    (pad 6 connect rect (at -15.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 7 /AD0))
    (pad 5 connect rect (at -17.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 6 /~CS_ROM))
    (pad 4 connect rect (at -18.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 5 /~RD))
    (pad 3 connect rect (at -20.25 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 4 /~WR))
    (pad 2 connect rect (at -21.75 0.25 270) (size 4.5 1) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 connect rect (at -23.4 0.5 270) (size 5 1.3) (layers F.Cu F.Mask)
      (net 2 VCC))
    (pad 32 connect rect (at 23.4 0.5 270) (size 5 1.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Package_SO:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5E476F32)
    (at 89.027 44.45 270)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (attr smd)
    (fp_text reference U1 (at 0 0.009 90) (layer F.SilkS))
    (fp_text value 74ALVC00 (at 0 3.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd roundrect (at 2.8625 -1.95 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 13 smd roundrect (at 2.8625 -1.3 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /U5-MAX))
    (pad 12 smd roundrect (at 2.8625 -0.65 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(U1-Pad12)"))
    (pad 11 smd roundrect (at 2.8625 0 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /U6-~EN))
    (pad 10 smd roundrect (at 2.8625 0.65 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /U4-MAX))
    (pad 9 smd roundrect (at 2.8625 1.3 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /U3-MAX))
    (pad 8 smd roundrect (at 2.8625 1.95 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /U5-~EN))
    (pad 7 smd roundrect (at -2.8625 1.95 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -2.8625 1.3 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /U4-~EN))
    (pad 5 smd roundrect (at -2.8625 0.65 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /U3-MAX))
    (pad 4 smd roundrect (at -2.8625 0 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /U3-MAX))
    (pad 3 smd roundrect (at -2.8625 -0.65 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~LD))
    (pad 2 smd roundrect (at -2.8625 -1.3 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /~CS_ROM))
    (pad 1 smd roundrect (at -2.8625 -1.95 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /~CS_ROM))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 59.818 47.4965 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0.7875 -1.5 90) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 43.434 47.3445 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -2.8945 -0.084 90) (layer F.SilkS))
    (fp_text value "100 nF" (at -0.8605 -1.884 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 60.518 29.984 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.163 -0.061 270) (layer F.SilkS))
    (fp_text value "100 nF" (at 0.2275 1.397 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 60.518 40.5215 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.0395 0.1 90) (layer F.SilkS))
    (fp_text value "100 nF" (at -0.2275 1.397 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 73.218 30.1465 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.7375 0.1 90) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 73.025 40.4465 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -3.2415 0 90) (layer F.SilkS))
    (fp_text value "100 nF" (at -4.45 0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 90.17 33.0465 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.9475 0 90) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-I-56_18.4x14mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 51.818 38.862 270)
    (descr "TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf)")
    (tags "TSOP I 32")
    (attr smd)
    (fp_text reference U7 (at 0 0 90) (layer F.SilkS))
    (fp_text value S29GL256S90T (at 0 8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 56 smd rect (at 9.75 -6.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 55 smd rect (at 9.75 -6.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 54 smd rect (at 9.75 -5.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /A16))
    (pad 53 smd rect (at 9.75 -5.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 52 smd rect (at 9.75 -4.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 9.75 -4.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /AD15))
    (pad 50 smd rect (at 9.75 -3.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /AD7))
    (pad 49 smd rect (at 9.75 -3.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /AD14))
    (pad 48 smd rect (at 9.75 -2.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /AD6))
    (pad 47 smd rect (at 9.75 -2.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /AD13))
    (pad 46 smd rect (at 9.75 -1.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /AD5))
    (pad 45 smd rect (at 9.75 -1.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /AD12))
    (pad 44 smd rect (at 9.75 -0.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /AD4))
    (pad 43 smd rect (at 9.75 -0.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 42 smd rect (at 9.75 0.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /AD11))
    (pad 41 smd rect (at 9.75 0.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /AD3))
    (pad 40 smd rect (at 9.75 1.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /AD10))
    (pad 39 smd rect (at 9.75 1.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD2))
    (pad 38 smd rect (at 9.75 2.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /AD9))
    (pad 37 smd rect (at 9.75 2.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 36 smd rect (at 9.75 3.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /AD8))
    (pad 35 smd rect (at 9.75 3.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD0))
    (pad 34 smd rect (at 9.75 4.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /~RD))
    (pad 33 smd rect (at 9.75 4.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 9.75 5.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /~CS_ROM))
    (pad 31 smd rect (at 9.75 5.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 /A0))
    (pad 30 smd rect (at 9.75 6.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at -9.75 6.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at -9.75 6.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -9.75 5.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /A1))
    (pad 25 smd rect (at -9.75 5.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /A2))
    (pad 24 smd rect (at -9.75 4.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /A3))
    (pad 23 smd rect (at -9.75 4.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /A4))
    (pad 22 smd rect (at -9.75 3.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /A5))
    (pad 21 smd rect (at -9.75 3.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /A6))
    (pad 20 smd rect (at -9.75 2.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 /A7))
    (pad 19 smd rect (at -9.75 2.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /A17))
    (pad 18 smd rect (at -9.75 1.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /A18))
    (pad 17 smd rect (at -9.75 1.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U7-Pad17)"))
    (pad 16 smd rect (at -9.75 0.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U7-Pad16)"))
    (pad 15 smd rect (at -9.75 0.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /A21))
    (pad 14 smd rect (at -9.75 -0.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 13 smd rect (at -9.75 -0.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /~WR))
    (pad 12 smd rect (at -9.75 -1.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /A20))
    (pad 11 smd rect (at -9.75 -1.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /A19))
    (pad 10 smd rect (at -9.75 -2.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 /A8))
    (pad 9 smd rect (at -9.75 -2.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /A9))
    (pad 8 smd rect (at -9.75 -3.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /A10))
    (pad 7 smd rect (at -9.75 -3.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 /A11))
    (pad 6 smd rect (at -9.75 -4.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /A12))
    (pad 5 smd rect (at -9.75 -4.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 /A13))
    (pad 4 smd rect (at -9.75 -5.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /A14))
    (pad 3 smd rect (at -9.75 -5.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /A15))
    (pad 2 smd rect (at -9.75 -6.25 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /A22))
    (pad 29 smd rect (at 9.75 6.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -9.75 -6.75 270) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /A23))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-I-56_18.4x14mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 66.548 42.545 270)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 74AC191 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /AD9))
    (pad 2 smd roundrect (at -2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /A9))
    (pad 3 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /A8))
    (pad 4 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /U5-~EN))
    (pad 5 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A10))
    (pad 7 smd roundrect (at -2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A11))
    (pad 8 smd roundrect (at -2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /AD11))
    (pad 10 smd roundrect (at 2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /AD10))
    (pad 11 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~LD))
    (pad 12 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /U5-MAX))
    (pad 13 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U5-Pad13)"))
    (pad 14 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /CLK))
    (pad 15 smd roundrect (at 2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /AD8))
    (pad 16 smd roundrect (at 2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 79.218 32.184 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0 0.006 90) (layer F.SilkS))
    (fp_text value 74AC191 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /AD4))
    (pad 14 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /CLK))
    (pad 13 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(U4-Pad13)"))
    (pad 12 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /U4-MAX))
    (pad 11 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~LD))
    (pad 10 smd roundrect (at 2.475 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /AD6))
    (pad 9 smd roundrect (at 2.475 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /AD7))
    (pad 8 smd roundrect (at -2.475 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /A7))
    (pad 6 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /A6))
    (pad 5 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /U4-~EN))
    (pad 3 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /A4))
    (pad 2 smd roundrect (at -2.475 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /A5))
    (pad 1 smd roundrect (at -2.475 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /AD5))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 79.018 42.545 270)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 74AC191 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /AD0))
    (pad 14 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /CLK))
    (pad 13 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(U3-Pad13)"))
    (pad 12 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /U3-MAX))
    (pad 11 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~LD))
    (pad 10 smd roundrect (at 2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /AD2))
    (pad 9 smd roundrect (at 2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /AD3))
    (pad 8 smd roundrect (at -2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /A3))
    (pad 6 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /A2))
    (pad 5 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /A0))
    (pad 2 smd roundrect (at -2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /A1))
    (pad 1 smd roundrect (at -2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AD1))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 87.518 31.684 270)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 0.015 90) (layer F.SilkS))
    (fp_text value 74LVC2G08 (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 7 smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 /CLK))
    (pad 6 smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 /U4-MAX))
    (pad 5 smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 63 /U3-MAX))
    (pad 4 smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad12)"))
    (pad 2 smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /~RD))
    (pad 1 smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /~WR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Fles (at 83.058 48.895) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 43.434 41.783 270) (layer B.SilkS))
  (gr_line (start 42.118 50.384) (end 64.318 50.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.318 50.384) (end 93.218 50.384) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 44.118 21.284) (end 44.118 20.384) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.518 21.284) (end 92.418 21.284) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.418 28.984) (end 92.418 21.284) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.518 28.984) (end 93.518 31.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.418 28.984) (end 93.518 28.984) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.118 20.384) (end 91.518 20.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 43.218 28.984) (end 43.218 21.284) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 42.118 28.984) (end 43.218 28.984) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 42.118 31.384) (end 42.118 28.984) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 67.818 50.384) (end 71.318 50.384) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.518 50.384) (end 93.318 50.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.518 31.384) (end 93.518 50.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.218 50.384) (end 93.318 50.384) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 42.118 31.384) (end 42.118 50.384) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.504 51.435) (xy 39.751 51.435) (xy 39.751 18.669) (xy 95.504 18.669)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.504 51.435) (xy 39.751 51.435) (xy 39.751 21.59) (xy 95.504 21.59)
      )
    )
  )
)
