FILE NAME:    ilo3_191.bin
TITLE:        Integrated Lights-Out 3 Firmware 1.91

LANGUAGE:  English

DIVISIONS:  Systems
PRODUCTS AFFECTED:
HP ProLiant BL685c G7 Server
HP ProLiant BL680c G7 Server
HP ProLiant BL620c G7 Server
HP ProLiant BL490c G7 Server
HP ProLiant BL465c G7 Server
HP ProLiant BL460c G7 Server
HP ProLiant BL2x220c G7 Server
HP ProLiant DL585 G7 Server
HP ProLiant DL580 G7 Server
HP ProLiant DL385 G7 Server
HP ProLiant DL380 G7 Server
HP ProLiant DL360 G7 Server
HP ProLiant DL120 G7 Server
HP ProLiant ML110 G7 Server
HP ProLiant ML10 G7 Server
HP ProLiant SL390s G7 Server
HP ProLiant SL335s G7 Server
HP ProLiant SL4545 G7 HyperStorage System

OPERATING SYSTEM:
Microsoft Windows Server 2012 R2      
Microsoft Windows Server 2012      
Microsoft Windows Server 2012 Essentials      
Microsoft Windows Server 2008 R2      
Microsoft Windows Server 2008 W32      
Microsoft Windows Server 2008 x64 
Microsoft Windows Server 2008 R2 Foundation Edition     
Microsoft Windows Server 2008 x64 - Server Edition     
Red Hat Enterprise Linux 7 Server 
Red Hat Enterprise Linux 6 Server (x86-64)      
Red Hat Enterprise Linux 6 Server (x86)      
Red Hat Enterprise Linux 5 Server (x86-64)      
Red Hat Enterprise Linux 5 Server (x86)      
SUSE Linux Enterprise Server 12      
SUSE LINUX Enterprise Server 11 
SUSE LINUX Enterprise Server 11 (x86)      
VMware vSphere 6.0     
VMware vSphere 5.5      
VMware vSphere 5.1      
VMware ESXi 5.0   

SYSTEM CONFIGURATION:  N/A

PREREQUISITE:  iLO 3 v1.90

BUILD DATE:  October 31, 2018

EFFECTIVE DATE:  November 8, 2018

DESCRIPTION:  Firmware for the Hewlett-Packard Integrated Lights-Out 3 Management Controller

LAST RECOMMENDED OR CRITICAL VERSION: 1.90

PREVIOUS VERSION: 1.90

UPGRADE REQUIREMENTS: RECOMMENDED

FIRMWARE DEPENDENCY: 

  Hewlett Packard Enterprise recommends upgrading to the minimum versions or later of the iLO 
  utilities:
  
  - HPQLOCFG v5.2 
  - Lights-Out XML Scripting Sample bundle 5.10.0
  - HPONCFG Windows 5.2.0
  - HPONCFG Linux 5.3.0
  - LOCFG v5.10.0
  - HPLOMIG 5.2.0

KNOWN ISSUES: 

- Intermittent authentication issues might occur when you use groups with a large number of Active Directory users.


ENHANCEMENTS:

- Adds the ability to enable and disable the iLO 3 webserver via the SSH command line interface.  The CLI commands “set /map1/config1 oemhp_httpport=0” or “set /map1/config1 oemhp_sslport=0” will disable the webserver.


SUPPORT:
- iLO 3 firmware updates and utilities can be found here:  http://www.hpe.com/support/ilo3
- IPv6 network communications - dedicated network connection only 
    Supported Networking Features 
    IPv6 Static Address Assignment 
    IPv6 SLAAC Address Assignment 
    IPv6 Static Route Assignment 
    Integrated Remote Console 
    OA Single Sign-On 
    Web Server 
    SSH Server 
    SNTP Client 
    DDNS Client 
    DHCPv6 Address Assignment 
    DHCPv6 Domain, DNS, and NTP Configuration 
    RIBCL over IPv6 
    HPE-SIM Single Sign-On 
    WinDBG Support 
    HPQLOCFG/HPLOMIG over an IPv6 connection
    Scriptable Virtual Media
    CLI/RIBCL Key Import over IPv6
    Authentication using LDAP and Kerberos over IPv6
    IPMI 

   Networking Features not supported by IPv6 in this release 
    Shared Network Port Connections  
    SNMP    
    NETBIOS-WINS

DOCUMENTATION:
- iLO 3 User Guide and iLO 3 Scripting and Command Line Guide can be found here:  http://www.hpe.com/support/ilo3
- Check the online help for additional information about how to use features.  Online help can be accessed from iLO web interface pages by clicking the question mark icon in the upper right-hand corner of each page.

HOW TO USE -
1. Download the appropriate iLO 3 Online Firmware Update Component for your operating system.
2. Install the firmware using one of these options:
    a) Run the component on the host to be updated. The component will update the iLO 3 firmware and reset the iLO processor.
    b) Extract the firmware from the component. This will place the firmware image file, iLo3_yyy.bin (where yyy represents the firmware version) in the target directory. You now have these options:
     i) Login to iLO, navigate to the Update Firmware page, and update the firmware from there.
     ii) Use the HP Lights-Out Configuration Utility (HPQLOCFG) and RIBCL/XML scripts to update iLO 3 across the network.
     iii) Use the HP Online Lights-Out Configuration utility (HPONCFG) and RIBCL/XML scripts to update iLO 3 from the supported host OS.
3. iLO automatically resets after a successful update. There is no need to manually reboot iLO.

Copyright 2018 Hewlett Packard Enterprise Development, LP