
	 Advanced Linux Sound Architecture  -  Supported SoundCards
	 ==========================================================

ID: SoundCard chipset/type
SC: SoundCard name
IF: Supported interfaces (MIXER,PCM,SYNTH,SYNTH_MIDI,SEQ,OPL,MIDI,EMUL,HWDEP)
MA: Maintainer
CO: Coder

This file is maintained by Jaroslav Kysela <perex@perex.cz>.
Note: OPL -> Raw (native) OPL
Note: MIDI -> external MIDI port
Note: EMUL -> MIDI emulation
Note: SYNTH -> yeah, well ?
Note: SYNTH_MIDI -> internal synth that handles MIDI data
Note: SEQ -> kernel client for ALSA sequencer
Note: HWDEP -> various hardware-dependent interfaces/devices
=====

ID: AMD InterWave
SC: Gravis UltraSound Plug & Play
SC: Dynasonic 3-D
SC: STB Sound Rage 32
SC: UltraSound 32-Pro (STB)
SC: MED3210
IF: MIXER,PCM,MIDI,SYNTH
MA: Jaroslav Kysela <perex@perex.cz>

ID: Gravis UltraSound MAX
IF: MIXER,PCM,MIDI,SYNTH
MA: Jaroslav Kysela <perex@perex.cz>

ID: Gravis UltraSound Extreme
SC: Synergy ViperMax
IF: MIXER,PCM,MIDI,SYNTH
MA: Jaroslav Kysela <perex@perex.cz>

ID: Gravis UltraSound Classic/ACE
IF: MIXER,PCM,SYNTH
MA: Jaroslav Kysela <perex@perex.cz>

ID: ESS AudioDrive ESx688
IF: MIXER,PCM,MIDI(1688)
MA: Jaroslav Kysela <perex@perex.cz>

ID: SoundBlaster 1.0/2.0/Pro
IF: MIXER (Pro only),PCM,MIDI
CO: Jaroslav Kysela <perex@perex.cz>
MA: Chris Butler <chrisb@sandy.force9.co.uk>

ID: SoundBlaster 16/AWE
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Yamaha OPL3-SA2/SA3
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: S3 SonicVibes PCI
SC: Schubert 32 PCI (PINE)
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Ensoniq AudioPCI (ES1370,ES1371)
SC: SoundBlaster PCI 64
SC: SoundBlaster PCI 128
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Cirrus Logic / Crystal Semiconductors CS4232/CS4232A
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Cirrus Logic / Crystal Semiconductors CS4235/CS4236/CS4236B/CS4237B/CS4238B/CS4239
SC: Turtle Beach Malibu
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Cirrus Logic / Crystal Semiconductors CS4281
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: Cirrus Logic / Crystal Semiconductors CS4610/CS4612/CS4614/CS4615/CS4622/CS4624/CS4280
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: ESS Solo-1 ES1938
IF: MIXER,PCM
MA: Jaromir Koutek <miri@punknet.cz>

ID: ESS ES18XX
IF: MIXER,PCM,MIDI
MA: Abramo Bagnara <abramo@alsa-project.org>

ID: OPTi 82C9xx
SC: Audio 16 Pro  EPC-SOUN9301      (82C930 based)
SC: ExpertColor  MED-3931 v2.0      (82C931 based)
SC: ExpertMedia Sound 16  MED-1600  (82C928 based - AD1848)
SC: Mozart  S601206-G               (OTI601 based - CS4231)
SC: Sound Player S-928              (82C928 based - AD1848)
IF: MIXER,PCM,OPL,MIDI
MA: Massimo Piccioni <dafastidio@libero.it>

ID: Trident 4DWave DX/NX
SC: Best Union  Miss Melody 4DWave PCI
SC: HIS  4DWave PCI
SC: Warpspeed  ONSpeed 4DWave PCI
SC: AzTech  PCI 64-Q3D
SC: Addonics  SV 750
SC: CHIC  True Sound 4Dwave
SC: Shark  Predator4D-PCI
SC: Jaton  SonicWave 4D
SC: Hoontech SoundTrack Digital 4DWave NX
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: ForteMedia FM801
SC: DT-0398
IF: MIXER,PCM,MIDI
MA: perex@perex.cz

ID: SGI Indy (HAL2)
IF: PCM
MA: Ulf Carlsson <ulfc@sgi.com>

ID: Turtle Beach WaveFront
SC: Tropez Plus (Tropez+)
SC: Tropez
SC: Maui (models with CS4232; others use OPTi 16 which is not handled)
IF: MIXER,PCM,MIDI,OPL,SYNTH_MIDI,HWDEP
CO: pbd@op.net
MA: pbd@op.net

ID: C-Media CMI8330
IF: MIXER,PCM
MA: George Talusan <gstalusan@uwaterloo.ca>

ID: C-Media CMI8338/8738
IF: MIXER,PCM,MIDI
MA: Takashi Iwai <tiwai@suse.de>

ID: Avance Logic ALS100/ALS120
IF: MIXER,PCM,MIDI
MA: Massimo Piccioni <dafastidio@libero.it>

ID: Diamond Technologies DT-019X
IF: MIXER,PCM,MIDI
MA: Massimo Piccioni <dafastidio@libero.it>

ID: Aztech Sound Galaxy
IF: MIXER,PCM,MIDI
MA: Christopher Butler <chrisb@sandy.force9.co.uk>

ID: Aztech AZF3328/PCI168
IF: MIXER,PCM,MIDI,OPL,SYNTH
MA: Andreas Mohr <hw7oshyuv3001@sneakemail.com>

ID: MOTU MidiTimePiece AV multiport MIDI interface
IF: MIDI
MA: Michael T. Mayers <tweakoz@pacbell.net>

ID: EMU10K1
SC: Sound Blaster Live!
SC: Sound Blaster PCI 512
SC: E-mu APS
IF: MIXER,PCM,MIDI,SYNTH_MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: RME Digi9652 (Hammerfall, Hammerfall light)
IF: PCM
MA: Paul Barton-Davis <pbd@op.net>

ID: Intel i810/i820/i830/i840/MX440
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>

ID: ESS Maestro 1/2/2E
IF: MIXER,PCM
MA: Matze Braun <MatzeBraun@gmx.de>

ID: VIA 82C686A (South Bridge)
IF: MIXER,PCM,MIDI
MA: Jaroslav Kysela <perex@perex.cz>
